Data/hora: 23/09/2024 19:41:54

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	22/12/1999	
Data da última atualização: 	22/12/1999	
Autoria: 	MATTOSO, L. H. C.; ZUCOLOTTO, V.; RAPOSO, M.; PONTES, R. S.; OLIVEIRA JUNIOR, O. N.	
Afiliação: 	EMBRAPA-CNPDIA; USP-IFSC; Uiversidade Nova de Lisboa-Faculdade de Ciencias e Tecnologia.	
Título: 	Adsorption process of self-assembled films of doped poly(o-methoxyaniline).	
Ano de publicação: 	1995	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON ORGANIZED MOLECULAR FILMS, 7., Sept. 1995, Numana, Ancona, Italia. Abstract book... [S.l.: s.n.], 1995.	
Páginas: 	p.57.	
Idioma: 	Inglês	
Notas: 	Ref.P-2.65.	
Conteúdo: 	An investigate is made of the fabrication process of self-assembled (SA) films of doped poly(o-methoxyaniline) alternated with polyacids. The buildup of bilayers is monitored by UV-vis spectroscopy and the absorbance is seen to increase linearly with the number of deposited layers. The kinetics of adsorption of each layer was also investigated. For the POMA layer a very short time period (3-5 min) suffices for complete adsorption to occur. Because adsorption is basically due to electrostatic interactions, we have probed the effects from applying electric fields on conducting glass and using charged Teflon substrates. In the latter case, successful SA film formation occurs. When electric fields are applied, however, the amount of doped POMA adsorbed increases but undesirable side effects appear such as the dedoping of the polymer which may hamper the buildup of multilayers.	
Palavras-Chave: 	Auto-montagem; filmes; Polianilina; Polyaniline; Self-assembled films.	
Thesagro: 	Absorção.	
Thesaurus Nal: 	adsorption.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (5499-1) - UPC - PL - -- - PROCI-95.00077 -  - 1995.00077 - DIS