Data/hora: 24/06/2024 05:45:36

Biblioteca(s): | Embrapa Milho e Sorgo.
Data corrente: | 11/06/2007
Data da última atualização: | 18/11/2015
Autoria: | KOMATUDA, A. S.; SANTOS, C. M. dos; SANTANA, D. G.; SOUZA, M. A. de; BRITO, C. H. de.
Título: | Influência de métodos de despendoamento na produtividade e na qualidade das sementes de milho.
Ano de publicação: | 2006
Fonte/Imprenta: | Revista Brasileira de Milho e Sorgo, Sete Lagoas, v. 5, n. 3, p. 359-368, 2006.
DOI: | http://dx.doi.org/10.18512/1980-6477/rbms.v5n3p359-368
Idioma: | Português
Conteúdo: | Em virtude da carência de pesquisas voltadas ao despendoamento mecanizado, o presente trabalho teve como objetivo comparar os métodos de despendoamento manual e mecanizado para a cultura do milho. A influência do despendoamento sobre a produtividade e a qualidade da semente foi estudada no híbrido ag 122, produzido pela Monsanto do Brasil Ltda. O experimento foi conduzido na fazenda Cachoeirinha, em Caiapônia (go), na safra de 2003/2004. O delineamento experimental utilizado foi o de blocos ao acaso, com seis tratamentos e quatro repetições. Os tratamentos constituíram-se de métodos de despendoamento, sendo quatro mecanizados (máquina com pneus regulada para remover 50%, 75% e 90% dos pendões, e com roçadeira, três dias antes da remoção de 75% dos pendões com pneus) e dois manuais (remoção apenas dos pendões e o padrão, removendo-se o ?cartucho?, ou seja, pendão com quatro a cinco folhas). O despendoamento mecanizado causou maiores danos às folhas superiores do milho, reduzindo em até 24,5% a produtividade, quando a máquina foi regulada para remoção de 90% dos pendões com os pneus; a remoção apenas do pendão alterou significativamente o vigor das sementes chatas, quando comparada ao despendoamento padrão, porém os métodos de despendoamento não influenciaram a germinação e o vigor das sementes de formato redondo. Due to the lack of research in mechanical detasseling, the present work was carried out to compare the manual and mechanical detasseling procedures. The detasseling influence on yield and seed quality was studied in AG 122 hybrid, produced by Monsanto do Brasil Ltda. This experiment was carried out in Cachoeirinha farm, at Caiapônia (GO), in the 2003/2004 growing season. The complete randomized-block experimental design was used, with six treatments and four replications. Treatments were comprised by six types of detasseling which were divided into four mechanical detasseling procedures (in the first three procedures, the machine?s tires were set to remove 50%, 75% and 90% of the tassels and the fourth had cutters applied to the second procedure (removal of 75% of the tassels with tires)) and two manual detasseling procedures (one with the removal of tassels only and the standard procedure, which consisted of removing tassels with four-to-five leaves). The mechanical detasseling caused more injuries to the upper leaves of the corn plant, leading to a 24.5% of seed yield reduction when the machine was regulated to remove 90% of the tassels with tires; the first manual procedure, i.e. the removal of tassel only, affected vigor of the flat seeds when compared to the standard procedure, but the procedures did not affect the germination and vigor of the round seeds.
Palavras-Chave: | Remoção do pendão.
Thesagro: | Milho Hibrido; Produção de Sementes; Zea Mays.
Categoria do assunto: | --
Registro original: | Embrapa Milho e Sorgo (CNPMS)
Exemplares: | CNPMS - (19914-1) - ADD - AP - DD -  -  -  - DIS