Data/hora: 23/09/2024 00:38:07

Biblioteca(s): 	Embrapa Milho e Sorgo; Embrapa Solos.	
Data corrente: 	28/10/2019	
Data da última atualização: 	27/01/2020	
Autoria: 	SALIS, H. H. C. de; COSTA, A. M. da; VIANA, J. H. M.; SCHULER, A. E.; KÜNNE, A.; FERNANDES, L. F. S.; PACHECO, F. A. L.	
Afiliação: 	Hugo Henrique Cardoso de Salis, Universidade Federal de Minas Gerais; Adriana Monteiro da Costa, Universidade Federal de Minas Gerais; JOAO HERBERT MOREIRA VIANA, CNPMS; AZENETH EUFRAUSINO SCHULER, CNPS; Annika Künne, University Jena; Luís Filipe Sanches Fernandes, Universidade de Trás-os-Montes e Alto Douro; Fernando António Leal Pacheco, Universidade de Trás-os-Montes e Alto Douro.	
Título: 	Hydrologic modeling for sustainable water resources management in urbanized Karst areas.	
Ano de publicação: 	2019	
Fonte/Imprenta: 	International Journal of Environmental Research and Public Health, v. 16, n. 14, article 2542, 2019.	
DOI: 	10.3390/ijerph16142542	
Idioma: 	Inglês	
Conteúdo: 	The potential of karst aquifers as a drinking water resource is substantial because of their large storage capacity gained in the course of carbonate dissolution. Carbonate dissolution and consequent development of preferential paths are also the reasons for the complex behavior of these aquifers as regards surface and underground flow. Hydrological modeling is therefore of paramount importance for an adequate assessment of flow components in catchments shaped on karsts. The cross tabulation of such components with geology, soils, and land use data in Geographic Information Systems helps decision makers to set up sustainable groundwater abstractions and allocate areas for storage of quality surface water, in the context of conjunctive water resources management. In the present study, a hydrologic modeling using the JAMS J2000 software was conducted in a karst area of Jequitiba River basin located near the Sete Lagoas town in the state of Minas Gerais, Brazil. The results revealed a very high surface water component explained by urbanization of Sete Lagoas, which hampers the recharge of 7.9 hm3 yr-1 of storm water. They also exposed a very large negative difference (-8.3 hm3 yr-1) between groundwater availability (6.3 hm3 yr-1) and current groundwater abstraction from the karst aquifer (14.6 hm3 yr-1), which is in keeping with previously reported water table declines around drilled wells that can reach 48 m in old wells used for public water supply. Artificial recharge of excess surface flow is not recommended within the urban areas, given the high risk of groundwater contamination with metals and hydrocarbons potentially transported in storm water, as well as development of suffosional sinkholes as a consequence of concentrated storm flow. The surface component could however be stored in small dams in forested areas from the catchment headwaters and diverted to the urban area to complement the drinking water supply. The percolation in soil was estimated to be high in areas used for agriculture and pastures. The implementation of correct fertilizing, management, and irrigation practices are considered crucial to attenuate potential contamination of groundwater and suffosional sinkhole development in these areas.	
Palavras-Chave: 	Gerenciamento sustentável; Modelagem hidrológica.	
Thesagro: 	Hidrologia; Recurso Hídrico; Zona Urbana.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/203842/1/Hydrologic-modeling.pdf	
Registro original: 	Embrapa Milho e Sorgo (CNPMS)	
Exemplares: 	CNPMS - (28964-1) - UPC - AP - DD -  -  -  - DIS
CNPS - (20278-1) - UPC - AP - DD -  -  - 2019.00188 - DIS