Data/hora: 20/06/2024 06:53:39

Biblioteca(s): 	Embrapa Solos.	
Data corrente: 	27/11/2018	
Data da última atualização: 	11/11/2021	
Autoria: 	TINTNER, J.; PREIMESBERGER, C.; PFEIFER, C.; SOLDO, D.; OTTNER, F.; WRIESSNIG, K.; RENNHOFER, H.; LICHTENEGGER, H.; NOVOTNY, E. H.; SMIDT, E.	
Afiliação: 	JOHANNES TINTNER, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; CHRISTOPH PREIMESBERGER, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; CHRISTOPH PFEIFER, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; DENIS SOLDO, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; FRANZ OTTNER, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; KARIN WRIESSNIG, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; HARALD RENNHOFER, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; HELGA LICHTENEGGER, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA; ETELVINO HENRIQUE NOVOTNY, CNPS; ENA SMIDT, UNIVERSITY OF NATURAL RESOURCES AND LIFE SCIENCES, VIENNA, AUSTRIA.	
Título: 	Impact of pyrolysis temperature on charcoal characteristics.	
Ano de publicação: 	2018	
Fonte/Imprenta: 	Industrial & Engineering Chemistry Research, v. 57, n. 46, p. 15613-15619, 2018.	
DOI: 	https://doi.org/10.1021/acs.iecr.8b04094	
Idioma: 	Inglês	
Conteúdo: 	Charcoals were produced from spruce and beech wood under laboratory conditions at different pyrolysis temperatures (300-1300 °C). Characterization of these charcoals was conducted using eight analytical methods. Each method describes specific changes in the temperature range until 1300 °C. Therefore, the combination of these methods provides comprehensive information on different pyrolysis stages. Fourier transform infrared (FTIR) spectroscopy, NMR spectroscopy, and thermogravimetry display changes until 700 °C. A prediction model for pyrolysis temperature until 800 °C is presented based on FTIR spectra with an R2 of 0.98. He-pycnometry resolves the temperature range between 500 and 890 °C. Small angle X-ray scattering (SAXS) describes precisely the evolution of the porous structure and completes the set of techniques by a description of the physical properties of the charcoal. X-ray diffraction (XRD) reveals the crystallographic change of the lignocellulosic structure toward precursors of graphite. The formation of calcite out of CaO and CO2 becomes evident.	
Thesagro: 	Carvão; Método de Análise.	
Thesaurus Nal: 	Charcoal; Pyrolysis.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Solos (CNPS)	
Exemplares: 	CNPS - (20019-1) - UPC - AP - DD -  -  - 2018.00306 - DIS