Data/hora: 23/09/2024 04:58:57

Biblioteca(s): 	Embrapa Milho e Sorgo.	
Data corrente: 	14/09/2020	
Data da última atualização: 	27/10/2020	
Autoria: 	SOUSA, S. S. de; FREITAS, D. A. F.; LATIN, A. O.; SILVA, B. M.; VIANA, J. H. M.; CAMPOS, M. P.; PEIXOTO, D. S.; BOTULA, Y.-D.	
Afiliação: 	Saulo Saturnino de Sousa, Universidade Federal de São João Del Rei; Diego Antônio França Freitas, Universidade Federal de São João Del Rei; Anderson Oliveira Latin, Universidade Federal de São João Del Rei; Bruno Montoani Silva, Universidade Federal de Lavras; JOAO HERBERT MOREIRA VIANA, CNPMS; Matheus Pena Campos, Universidade Federal de São João Del Rei; Devison Souza Peixoto, Universidade Federal de Lavras; Yves?Dady Botula, University of Quebec in Abitibi-Temiscamingue.	
Título: 	Iron ore mining areas and their reclamation in Minas Gerais State, Brazil: impacts on soil physical properties.	
Ano de publicação: 	2020	
Fonte/Imprenta: 	SN Applied Sciences, v. 2, e1659, 2020.	
DOI: 	https://doi.org/10.1007/s42452-020-03457-9	
Idioma: 	Inglês	
Notas: 	Publicado online em 9 set. 2020.	
Conteúdo: 	Plant cover acts to maintain the balance between soil chemical, physical, and biological attributes, as well as superfcial soil protection. The aim of this study was to evaluate the impacts of iron ore mining and their reclamation on soil physical properties and soil visual quality in Fort Lauderdale Municipal Park and Serra do Curral Municipal Park, Iron Quadrangle (Quadrilátero Ferrífero), Minas Gerais State, Brazil. The evaluated areas varied in relation to the post-mining condition, natural revegetation (NR), an area with gully erosion (GA) and area under eucalyptus revegetation (ER) and native vegetation cover, rupestrian feld (RF), and seasonal semi-deciduous forest (NF). The main soil physical attributes evaluated were: soil organic matter (SOM), geometric mean diameter (GMD), weighted mean diameter (WMD), bulk density (Bd), air capacity (ACb), plant-available water capacity (AWC), relative feld capacity (RFC), and visual soil quality assessment. In addition to the impacts on the landscape, with removal of vegetation and soil cover, iron ore mining process impacts soil physical quality measured through porosity and aggregation properties and therefore could impact ecosystems services. Areas of iron post-mining that are not restored can develop gully erosion. NR shows high erosion risk inferred through aggregation indicators (GMD=3.84 mm; MWD=3.04 mm), despite similar soil organic matter content and higher plant-available water and air (NR [AWC=0.102 m3 m&#8722;3; ACb=0.328 m3 m&#8722;3], NF [AWC=0.062 m3 m&#8722;3; ACb=0.202 m3 m&#8722;3]) compared with NF (GMD=4.77 mm; MWD=4.56 mm). ER had similar soil structure stability compared to NF as well most of the porosity indicators, which is associated with the higher soil organic matter. Soil visual assessment alone was not able to characterize the soil physical quality, mainly in the post-mining areas, because it was designed for agricultural soils.	
Palavras-Chave: 	Avaliação ambiental; Degradação do solo; Quadrilátero Ferrífero.	
Thesagro: 	Biomassa; Contaminação; Degradação Ambiental; Impacto Ambiental; Metal Pesado; Mineração; Saúde; Solo; Sorgo.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/215954/1/Iron-mining.pdf	
Registro original: 	Embrapa Milho e Sorgo (CNPMS)	
Exemplares: 	CNPMS - (29352-1) - UPC - AP - DD -  -  -  - DIS