Data/hora: 22/06/2024 00:26:35

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 21/01/2005
Data da última atualização: | 08/03/2010
Autoria: | VAZ, C. M. P.
Título: | Automatic gamma-ray equipment for multiple soil physical properties measurements.
Ano de publicação: | 2004
Fonte/Imprenta: | In: Invited presentations college on soil physics 2003. [Trieste]: s.n., 2004. p. 461-468.
Série: | (ictp lecture notes, 18)
Idioma: | Inglês
Notas: | Editores: GABRIELS, D. M. ; GHIRARDI, G. ; NIELSEN, D. R. ; SENTIS, I. P. ; SKIDMORE, E. L.
Conteúdo: | Determination of solphysical parameters is sometimes very laborious and time consuming. For instance, the soil water retention curve takes several weeks. Participle density by picnometer and granulmetry (texture) by pipette method are laborious methods. Other parameters, such as bulk density and total porosity, are determined by gravimetric methods and depends on oven drying the samples for 24 hours.
Thesagro: | Física do Solo; Solo.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (8606-1) - UPC - SP - -- - PROCI-04.00094 -  - 2004.00094 - DIS