Data/hora: 20/06/2024 02:06:19

Biblioteca(s): | Embrapa Agricultura Digital; Embrapa Agrossilvipastoril.
Data corrente: | 18/02/2021
Data da última atualização: | 02/12/2021
Autoria: | KAMCHEN, S. G.; SANTOS, E. F. dos; LOPES, L. B.; VENDRUSCULO, L. G.; CONDOTTA, I. C. F. S.
Afiliação: | SCHEILA GEIELE KAMCHEN, UFMT, Cuiaba-MT; ELTON FERNANDES DOS SANTOS, UFMT, Sinop-MT; LUCIANO BASTOS LOPES, CPAMT; LAURIMAR GONCALVES VENDRUSCULO, CNPTIA; ISABELLA C. F. S. CONDOTTA, University of Illinois.
Título: | Application of depth sensor to estimate body mass and morphometric assessment in Nellore heifers.
Ano de publicação: | 2021
Fonte/Imprenta: | Livestock Science, v. 245, 104442, 2021.
ISSN: | 1871-1413
DOI: | https://doi.org/10.1016/j.livsci.2021.104442
Idioma: | Inglês
Conteúdo: | Abstract. The potential of an RGB-D sensor as a tool to estimate Nellore heifers´ body mass and morphometric measurements through image analysis was evaluated. An Intel RealSense D435i depth sensor was used to acquire dorsal images of 260 animals aged between 8 and 18 months. Images were acquired from March to December 2019 in six-time points. The best quality images were selected using a multi-layer perceptron neural network (nn = 547). The images were then manually associated with each animal's electronic ear tag. Morphometric measurements were manually acquired using a hipometer and measured on the images using the OpenCV library's graphical interface. These values were acquired in pixels converted to meters. The adjusted linear regression analysis between body mass measured with a scale and estimated body volume presented a high coefficient of determination of R² = 0.97. The mean absolute percentage error was 3.13%, the absolute error was ± 8.85 kg, and the mean squared error was 10.07 kg. The mean absolute error, mean squared error and mean absolute percentage error between manually acquired and digitally acquired morphometric measurements were: 4.23 cm, 5.34 cm, and 18% for chest width (R² = 0.56); 4.4 cm, 5.1 cm, and 13.9% for croup width (R² = 0.86); 6.0 cm, 8.0 cm, and 19.3% for croup length (R² = 0.75); 4.7 cm, 6.6 cm, and 3.8% for croup height (R² = 0.9); and 3.5 cm, 5.1 cm, and 2.9% for withers height (R² = 0.92). This study showed that it is possible to estimate body mass in Nellore heifers using a depth sensor and has good potential for application on morphometric evaluations.
Palavras-Chave: | Análise de imagem; Massa corporal; Nellore heifers´ body mass; Novilhas Nelore; Pecuária de precisão; Precision livestock farming; RealSense D435i; Sensor RGB-D.
Thesagro: | Gado; Gado Nelore.
Thesaurus Nal: | Body mass index; Cattle; Heifers; Image analysis.

Categoria do assunto:

--
X Pesquisa, Tecnologia e Engenharia

Registro original: | Embrapa Agrossilvipastoril (CPAMT)

Exemplares:

CNPTIA - (20897-1) - UPC - AP - DD -  -  -  - DIS
CPAMT - (1649-1) - UPC - AP - DD -  -  -  - DIS