Data/hora: 23/06/2024 17:29:42

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 30/03/2006
Data da última atualização: | 24/08/2010
Autoria: | ASSIS, O. B. G.; VIEIRA, D. C.
Título: | Processing of open-pore glass membranes with defined pores form.
Ano de publicação: | 2000
Fonte/Imprenta: | In: ANNUAL MEETING E EXPOSITION, 102., 2000, St. Louis. Annual meeting abstracts... Westerville: American Ceramic Society, 2000. p. 340.
Idioma: | Inglês
Conteúdo: | The development of open-pore glass membranes with defined pore geometry, suitable to enzyme immobilization, is processed following the efiller principleí. In this process an inorganic, non-sinterizable water-soluble phase, is admixed as pore-forming agents. After the heating cycle the salt is washed out forming a continuous porous structure.
Palavras-Chave: | AFM; Membranas; Open-pore; SEM.
Thesagro: | Enzima.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9701-1) - UPC - SP - -- - PROCI-00.00009 -  - 2000.00009 - DIS