Data/hora: 19/05/2024 18:05:27

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 28/03/2005
Data da última atualização: | 20/06/2018
Autoria: | PEDROTTI, A.; PAULETTO, E. A.; CRESTANA, S.; CRUVINEL, P. E.; VAZ, C. M. P.; NAIME, J. M.; SILVA, A. M.
Título: | Planosol soil sample size for computerized tomography measurement of physical parameters.
Título original: | Tamanho de amostras para a determinação de parâmetros físicos em planossolo por tomografia computadorizada.
Ano de publicação: | 2003
Fonte/Imprenta: | Scientia Agricola, v. 60, n. 4, p. 735-740, 2003.
Idioma: | Inglês
Conteúdo: | Computerized tomography (CT) is an important tool in Soil Science for noninvasive measurement of density and water content of soil samples. This work aims to describe the aspects of sample size adequacy for Planosol (Albaqualf) and to evaluate procedures for statistical analysis, using a CT scanner with a 241Am source. Density errors attributed to the equipment are 0.051 and 0.046 Mg m-3 for horizons A and B, respectively. The theoretical value for sample thickness for the Planosol, using this equipment, is 4.0 cm for the horizons A and B. The ideal thickness of samples is approximately 6.0 cm, being smaller for samples of the horizon B in relation to A. Alternatives for the improvement of the efficiency analysis and the reliability of the results obtained by CT are also discussed, and indicate good precision and adaptability of the application of this technology in Planosol (Albaqualf) studies.
Palavras-Chave: | Amostras; Determinação de parâmetros; Tomografia computadorizada.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (8769-1) - UPC - SP - -- - PROCI-03.00114 -  - 2003.00114 - DIS