Data/hora: 16/05/2024 15:18:13

Biblioteca(s): | Embrapa Meio Norte / UEP-Parnaíba.
Data corrente: | 12/02/1996
Data da última atualização: | 12/02/1996
Autoria: | WHITE, R. E.
Afiliação: | University of Oxford.
Título: | A model for nitratre leaching in undisturbed structured clay soil during unsteady flow.
Ano de publicação: | 1985
Fonte/Imprenta: | Journal of Hydrology, v.79, p.37-51, 1985.
Idioma: | Inglês
Conteúdo: | A two-domain mixing model is described for predicting nitrate leaching during unsteady unsaturated flow through soil. The model assumes that water infiltrating the soil surface mixes incompletely with resident water to form a miscible transport volume, the size of which can vary with time. Changes in solute storage within the transport volume can occur by diffusion and biological transformations. Output from the transport volume is by drainage from a lower surface in the soil. The model's output was tested against the measured amounts of NO3-N leached from large undisturbed cores of structured clay soil during constant flux irrigation with 10 mM CaCl2. The average concentration of NO-3 and Cl- in the soil solution was determined by extraction of smallcores taken around the large cores prior to leaching. The rate of nitrification in the soil was also measured. The change in the transport volume with time was calculated from equations for the mass balance of water and Cl- in the transport volume. Knowing the transport volume, analogous equations in terms of NO-3 were solved to predict the NO-3 concentration in the effluent. Good agreement between predicted and observed NO3-N leached was obtained for cores showing divergent trends in NO-3 leaching. A large difference between cores in the fraction of soil NO3-N leached (0.34 compared to 0.13) was attributed to the difference in the volume of high-nitrate soil water that mixed with infiltrating water to form the transport volume, and to differences in...
Palavras-Chave: | Chloride; Lixiviacao de nitrato; Nitrate; Nitrate leaching.
Thesagro: | Argila; Cloreto; Drenagem; Lixiviação; Nitrato.
Thesaurus Nal: | clay; drainage; leaching.
Categoria do assunto: | --
Registro original: | Embrapa Meio Norte / UEP-Parnaíba (CPAMN-UEPP)
Exemplares: | CPAMN-UEPP - (5018-1) - ADP - SP - -- -  -  - 1993.04838 - DIS