Data/hora: 26/07/2024 22:16:04

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	29/09/2005	
Data da última atualização: 	29/09/2005	
Autoria: 	MALMONGE, J. A.; CAMPOLI, C. S.; MATTOSO, L. H. C.	
Título: 	Eletrically conductive blends of polyurethane and polyaniline.	
Ano de publicação: 	2001	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON FRONTIERS OF POLYMERS ADVANCED MATERIALS, 6., 2001, Jaboatão dos Guararapes. Technical digest: conference & exhibition: a conference on advanced materials, emerging new technologies and business opportunities. Recife: Universidade Federal de Pernambuco; Buffalo: State University of New York, 2001. p. 107 ref. TuPC22.	
Idioma: 	Inglês	
Conteúdo: 	Free standing films of blends from Polyurethane (PU) and polyaniline (PANI) were obtained casting and characterized by the two probe conductivity, in a sandwich configuration with gold electrodes, ultraviolet-visible-near infrared (UV-Vis-NIR) spectoscopy and scanning electronic microscopic (SEM).	
Palavras-Chave: 	Condutividade; Polianilina; Polímeros.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8987-1) - UPC - SP - -- - PROCI-01.00082 -  - 2001.00082 - DIS