Data/hora: 18/06/2024 13:20:20

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	29/03/2006	
Data da última atualização: 	29/03/2006	
Autoria: 	ASSIS, O. B. G.; CLARO, L. C.	
Título: 	Processing of soda lime glass membranes by filler principle and enzyme immobilization by S.A. technique.	
Ano de publicação: 	1998	
Fonte/Imprenta: 	In: BRAZILIAN SYMPOSIUM ON GLASSES AND RELATED MATERIALS, 3., 1998, Bonito, MS. Program and abstracts... [S.l.: s.n], 1998. p. 75. Ref. PS13.	
Idioma: 	Inglês	
Conteúdo: 	High chemical resistance materials as glass porous membranes become increasingly interesting with respect to applications in pharmaceutics, medicine and biotechnology. In particular the possibility to enhance filtration effectiveness by combination of conventional separation process and biological catalysis by use of immobilized enzymes is a very desired clean-up technology. In this work is presented and discussed aspects of manufacture and microstructure of open-pore sintered soda lime glasses, as well as the appropriated surface treatment for enzymes immobilization.	
Palavras-Chave: 	Open-pore; Soda limão.	
Thesagro: 	Biotecnologia; Enzima.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9685-1) - UPC - SP - -- - PROCI-98.00006 -  - 1998.00006 - DIS