Data/hora: 11/06/2024 18:04:03

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	20/02/2006	
Data da última atualização: 	20/02/2006	
Autoria: 	ALVES, C. R.; ASSIS, O. B. G.	
Título: 	Surface modification of ceramic household filtration candles by SiO2 sol-gel film coatings.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	In: INTERNATIONAL LATIN-AMERICAN CONFERENCE ON POWDER TECHNOLOGY-PTECH, 2., 1999, Foz do Iguaçu. PTECH' 99: Powder technology: challenges for the next millenium. [S.l.]: Associação Brasileira de Cerâmica, 1999. Não paginado, ref. CO45.	
Idioma: 	Inglês	
Conteúdo: 	In this work we used the sol-gel technique to obtain SiO2 film onto commercial household ceramic filter candles. The main aim here is to increment the wetting characteristics of these elements by increasing of Si density on the pore's surfaces. Since the number of silanois sites (SiOH) can define the degree of hydrophilization, these sites can be chemically activated to become appropriated as substrate for the immobilization of organic agents.	
Palavras-Chave: 	EDX; SEM; SiOH; TMOS.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9412-1) - UPC - SP - -- - PROCI-99.00002 -  - 1999.00002 - DIS