Data/hora: 02/06/2024 15:45:24

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	20/02/2006	
Data da última atualização: 	20/02/2006	
Autoria: 	ALVES, C. R.; ASSIS, O. B. G.	
Título: 	SEM and EDX characterization of sol-gel SiO2 film on porous ceramic substrate.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	Acta Microscopica, Rio de Janerio, v. 8, Suppl. A, p. 319-320, Oct. 1999. Edição de P)roceedings of the XVII Congress of the Brazilian Society for Cell Biology for Microscopy and Microanalysis; X Congress of the Brazilian Society for Cell Biology held in Santos, SP, Oct. 1999. Resumo.	
Idioma: 	Inglês	
Conteúdo: 	Commercial filters based on alumina-silicate ceramic, were used as substrates for SiO2 film deposition using the sol-gel technique. The main aim of this work is to increment the degree of hydrophilization by an increase of the Si density on the pore's surfaces. The hydrophilization is an important property to water-filters and can be defined by the silanois sites (SiOH) on the surface.	
Palavras-Chave: 	Alumina-silicate ceramic; Hidrofilização; TMOS.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9413-1) - UPC - SP - -- - PROCI-99.00003 -  - 1999.00003 - DIS