Data/hora: 23/09/2024 01:46:24

Biblioteca(s): 	Embrapa Gado de Leite.	
Data corrente: 	06/07/2017	
Data da última atualização: 	30/01/2023	
Autoria: 	MEURER, I. R.; LANGE, C. C.; HUNGARO, H. M.; BELL, M. J. V.; ANJOS, V. de C. dos; SILVA, C. A. de S.; PINTO, M. A. de O.	
Afiliação: 	Igor Rosa Meurer, UFJF; CARLA CHRISTINE LANGE, CNPGL; Humberto Moreira Hungaro, UFJF; Maria Jose Valenzuela Bell, UFJF; Virgilio de Carvalho dos Anjos, UFJF; Cleuber Antonio de Sa Silva, IF-SUDESTE, Rio Pomba, MG; Miriam Aparecida de Oliveira Pinto, UFJF.	
Título: 	Quantification of whole ultra high temperature UHT milk waste as a function of packages type and design.	
Ano de publicação: 	2017	
Fonte/Imprenta: 	Journal of Cleaner Production, v. 153, p. 483-490, 2017.	
Idioma: 	Inglês	
Conteúdo: 	The food waste during consumption should be decreased to assure environmental sustainability and food safety. Packages play an important role in the preservation of quality and safety of food, but their design is related with food waste. The Ultra High Temperature (UHT) milk residue remaining inside the packages after consumption is an example of this condition. The purpose of this work was to quantify and analyze the factors influencing the whole UHT milk waste, as a function of its packages. Ten different types of one liter packages were analyzed, and a descriptive study of their characteristics has been developed according to package material, type of opening, and their dimensions. A method for quantification of UHT milk waste in the analyzed packages was developed. The waste was quantified by means of gravimetric analysis and volume conversion under two conditions: WITHOUT and WITH packages stirring after their deflation. A large variation in the wasted volume of milk was observed for the different types of package under both tested conditions. The package stirring process has significantly influenced the waste decrease in five different types of package. It was observed that the package design directly influences the UHT milk waste, mainly due to folding at package bottom, corrugations in its internal wall and kind of opening of the packages. The values of wasted milk ranged from (0.43 ± 0.03) to (7.7 ± 0.4) ml and (0.51 ± 0.04) to (14.7 ± 0.4) ml for the WITH and WITHOUT stirring, respectively. Thus, the choice of packaging showing suitable design for complete emptying of the content may reduce the UHT milk waste contributing to the food safety and environmental protection.	
Palavras-Chave: 	Package; Waste.	
Thesaurus Nal: 	environment; food safety; UHT milk.	
Categoria do assunto: 	Q Alimentos e Nutrição Humana	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (23571-1) - UPC - AP - DD -  -  -  - DIS