Data/hora: 19/06/2024 21:35:30

Biblioteca(s): | Embrapa Cerrados.
Data corrente: | 04/03/2016
Data da última atualização: | 04/03/2016
Autoria: | HERMES, E.; VILAS BOAS, M. A.; RODRIGUES, L. N.; MELO, E. L. de; GONÇALVES, M. P.; LINS, M. A.; BERGER, J. S.
Afiliação: | LINEU NEIVA RODRIGUES, CPAC.
Título: | Process capacity index in drip irrigation with cassava wastewater processing.
Ano de publicação: | 2015
Fonte/Imprenta: | African Journal of Agricultural Research, v. 10, n. 2, p. 1427-1433, Mar. 2015.
DOI: | http://dx.doi.org/10.5897/AJAR2015.9610
Idioma: | Português
Conteúdo: | The study aimed to evaluate the performance of drip irrigation systems with clean water application and cassava wastewater processing, by determining the distribution uniformity coefficient (CUD) and the process capability index (Cpl). The research was carried out in an agroindustrial area from western Paraná State, Brazil, where two irrigation systems were set and operated in different periods. After the essays implementation, the two irrigation systems were identified and stored in order to be retested after one year (2nd year of collection). So, the same conditions that were established in the first year had still been considered. Treatments with effluent showed flow averages near to those ones obtained with the use of clean water. Only in the T4 treatment, CUD was classified as good, while the others were excellent. The process was rated as efficient only in T1 with 80% LCL, with a 2.04 Cpl. Thus, based on this technique, it was possible to check that the system is able to keep suitable levels of uniformity.
Palavras-Chave: | Distribution uniformity; Process capability.
Thesaurus Nal: | water quality.
Categoria do assunto: | P Recursos Naturais, Ciências Ambientais e da Terra
Registro original: | Embrapa Cerrados (CPAC)
Exemplares: | CPAC - (35264-1) - UPC - SP - PP - S2116 -  - S2116 - DIS