Data/hora: 19/06/2024 14:57:50

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 21/02/2006
Data da última atualização: | 21/02/2006
Autoria: | ASSIS, O. B. G.; CLARO, L. C.
Título: | Processing of soda-lime glass membranes by filler principle for the enzyme coupling applications.
Ano de publicação: | 1999
Fonte/Imprenta: | Journal of Non-Crystalline Solids, Amsterdam, v. 247, p. 237-240, 1999.
Idioma: | Inglês
Conteúdo: | Open-pore soda-lime glass membranes were processed following the filler principle. In this process salt is homogeneously mixed with glass powder and acts as an inorganic non-sinterizable additive. The salt is then removed and a continuous porous structure is formed. The microstructure of the final sintered and washed compacts was evaluated using scanning electron microscopy and found to be dependent on the features of the inorganic solvent. The main por configuration is that of the pores formed is favorable to a homogeneous enzyme deposition of which interconnection features improve the contact of the liquid and the reactie immobilized film.
Palavras-Chave: | Enzimas; Membranas; Open-pore.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9426-1) - UPC - SP - -- - PROCI-99.00008 -  - 1999.00008 - DIS