Data/hora: 17/06/2024 03:38:28

Biblioteca(s): 	Embrapa Meio Ambiente.	
Data corrente: 	16/01/2018	
Data da última atualização: 	16/01/2018	
Autoria: 	ROMERO, D. J.; BEN-DOR, E.; DEMATTÊ, J. A. M.; SOUZA, A. B. e; VICENTE, L. E.; TAVARES, T. R.; MARTELLO, M.; STRABELI, T. F.; BARROS, P. P. da S.; FIORIO, P. R.; GALLO, B. C.; SATO, M. V.; EITELWEIN, M. T.	
Afiliação: 	DANILO JEFFERSON ROMERO, ESALQ-USP; EYAL BEN-DOR, Tel Aviv University; JOSÉ ALEXANDRE MELO DEMATTÊ, ESALQ-USP; ARNALDO BARROS E SOUZA, ESALQ-USP; LUIZ EDUARDO VICENTE, CNPMA; TIAGO RODRIGUES TAVARES, ESALQ-USP; MAURICIO MARTELLO, ESALQ-USP; TAILA FERNANDA STRABELI, ESALQ-USP; PEDRO PAULO DA SILVA BARROS, ESALQ-USP; PETERSON RICARDO FIORIO, ESALQ-USP; BRUNA CRISTINA GALLO, ESALQ-USP; MARCUS VINOCIUS SATO, ESALQ-USP; MATEUS TONINI EITELWEIN, ESALQ-USP.	
Título: 	Internal soil standard method for the Brazilian soil spectral library: performance and proximate analysis.	
Ano de publicação: 	2018	
Fonte/Imprenta: 	Geoderma, v. 312, p. 95-103, 2018.	
ISSN: 	0016-7061	
DOI: 	http://dx.doi.org/10.1016/j.geoderma.2017.09.014	
Idioma: 	Inglês	
Conteúdo: 	There are several methods to extract soil information by spectral sensing. For this reason, the database should be built including standards and protocols both in the lab and in &#64257;eld acquisitions. If we does not align the measurement one to each other, the models will have no merit in term of large-scale application and stay as an academic exercise only. The use of standard samples with known spectra is expected to allow parameterizing mathematically soil spectra collected by di&#64256;erent equipment and with distinct geometries. This study was proposed for the reason that to date, the new methodology proposed has not been evaluated in Brazilian tropical soils (Oxisols) in visible, near and short infrared (VIS-NIR-SWIR ? 350 to 2500 nm) spectral regions from three spectrometers (FieldSpec 3) in three distinct protocols (Long Light, Near Light and Contact Probe). The current study compared the spectral intensity of each combination between spectrometers and protocols by ANOVA module and the clay prediction capacity by PLSR with cross-validation, before and after the internal soil standard (ISS) method application. The results showed that visual spectral variation is minimized by the ISS method and its correction enables better proxy modeling of clay content especially if the data are mixed from di&#64256;erent protocols. The model for clay prediction was improved showing a favorable case to use the ISS technique in any soil spectral measurement in a better way to merge spectral libraries from di&#64256;erent sources.	
Palavras-Chave: 	Clay prediction; Soil measurement protocol; Soil spectroscopy; VIS-NIR-SWIR.	
Thesagro: 	Análise do solo; Argila; Oxisol; Sensoriamento remoto; Solo tropical.	
Thesaurus Nal: 	Remote sensing; Soil analysis; Soil surveys.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Meio Ambiente (CNPMA)	
Exemplares: 	CNPMA - (15968-1) - UPC - AP - DD -  -  -  - DIS