Data/hora: 25/06/2024 15:04:09

Biblioteca(s): | Embrapa Agroenergia.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | B - 1
Data corrente: | 03/11/2015
Data da última atualização: | 20/09/2017
Autoria: | VAZ JUNIOR, S.; DONATE, P. M.
Afiliação: | SILVIO VAZ JUNIOR, CNPAE; Paulo Marcos Donate, USP.
Título: | Microwave-assisted green production of furfural from D-xylose of sugar cane bagasse.
Ano de publicação: | 2015
Fonte/Imprenta: | BioResources. n. 10 v. 4, 2015
DOI: | 10.15376/biores.10.4.8168-8180
Idioma: | Inglês
Conteúdo: | D-xylose is a component of sugarcane bagasse that can be used as a renewable resource for the production of a variety of chemicals. By means of catalytic reactions in an aqueous medium, it was determined that D-xylose can efficiently be converted into furfural by the application of microwave as a green synthetic methodology. The highest yields of furfural were obtained at a HCl concentration of 4 mg/mL. When the reaction was performed at 200 °C, an optimum yield of 64% of furfural was observed after 10 min of reaction time, with 95% of the D-xylose being converted.
Palavras-Chave: | Green processes; Renewable chemistry.
Thesaurus Nal: | green chemistry.
Categoria do assunto: | --
Registro original: | Embrapa Agroenergia (CNPAE)
Exemplares: | CNPAE - (2736-1) - UPC - AP - DD -  -  -  - DIS