Data/hora: 01/06/2024 21:45:34

Biblioteca(s): | Embrapa Uva e Vinho.
Tipo da produção científica: | Artigo em Anais de Congresso
Data corrente: | 20/12/2018
Data da última atualização: | 20/12/2018
Autoria: | BERNARDELLI, P. V.; MAGRO, P.; NAGEL-HASSMER, M. E.; GEBLER, L.
Afiliação: | Priscilla Veiga Bernardelli, Universidade Federal de Santa Catarina; Paulo Magro, Universidade Federal de Santa Catarina; Maria Eliza Nagel-Hassmer, Universidade Federal de Santa Catarina; LUCIANO GEBLER, CNPUV.
Título: | Processo oxidativo avançado (UV/H2O2) como alternativa de pré-tratamento de efluente contaminado pelo agrotóxico clorpirifós.
Ano de publicação: | 2018
Fonte/Imprenta: | In:CONGRESSO INTERAMERICANO DE INGENIERÍA SANITARIA Y AMBIENTAL, 26., 2018. Libros de Trabajos Técnicos: Posters...Guayaquil, Ecuador: AIDIS, 28 a 31 Oct. 2018. [00230].
Idioma: | Inglês
Conteúdo: | Brazil has become the world?s top pesticide consumer since 2008. This high consumption rate could lead to serious environmental, sanitary and social risks. Given this, mitigating practices play a fundamental role to reduce the impact caused by pesticide use. Among these, a bioreactor known as Biobed stands out. However, some specific pesticides interfere negatively on that reactor, consequently diminishing its efficiency. In this context, the Advanced Oxidation Process UV/H2O2 proves to be an interesting pretreatment alternative, as it has shown to be effective for different pesticides degradation. The aim of this study was to evaluate UV/H2O2 technology as a chlorpyrifos pretreatment, in order to determine the pre-oxidation conditions. The photodegradation was carried out in an annular reactor, with a high pressure UV lamp. Tests were performed with the initial H2O2 concentration varying from 600 to 2000 mg/L and reaction time from 15 to 80 minutes, while the lamp was powered both with 80 and 125W. The best result was obtained using 125W, H2O2 concentration of 1750 mg/L and 80 minutes of pre-oxidation, providing a 31.5% removal. These results show that UV/H2O2 technology is efficient as a pretreatment technique, resulting in a less concentrated and toxic effluent, so it could be further degraded by bioreactors. Palavras-chave: Pré-tratamento, UV/H2O2 , Biobed
Palavras-Chave: | Biobed; Pré-tratamento; UV/H2O2.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/189176/1/AIDIS-2018-Libro-Trabajos-Tecnicos-Carteles-00230.pdf
Registro original: | Embrapa Uva e Vinho (CNPUV)
Exemplares: | CNPUV - (18020-1) - UPC - AA - DD -  -  - 18.02412 - DIS