Data/hora: 24/06/2024 15:30:32

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	05/04/2005	
Data da última atualização: 	05/04/2005	
Autoria: 	MEDEIROS, E. S.; AGNELLI, J. A. M.; JOSEPH, K.; CARVALHO, L. H.; MATTOSO, L. H. C.	
Título: 	Curing behavior of a Novolac-type phenolic resin analyzed by differential scanning calorimetry.	
Ano de publicação: 	2003	
Fonte/Imprenta: 	Journal of applied polymer science, v. 90, p.g 1678-1682, 2003.	
Idioma: 	Inglês	
Conteúdo: 	Phenolic resins are widely used condensation poly- mers because of their high chemical resistance, electri- cal insulation, and dimensional stability. Their roain applications include molding materiaIs, laminates, and adhesives in the manufacture of plywood.1 
There are two major categories of phenolic resins that are classified by their structures and curing prop- erties as resole or novolac. The essential characteristics of both cured resole and novolac-type phenolic resins are almost identical (e.g., mechanical properties, chemical resistance, etc.).	
Palavras-Chave: 	DSC; Método Ozawa; Microgel; Resinas fenólicas.	
Thesaurus Nal: 	differential scanning calorimetry.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8786-1) - UPC - SP - -- - PROCI-03.00131 -  - 2003.00131 - DIS