Data/hora: 06/06/2024 03:49:24

Biblioteca(s): 	Embrapa Florestas.	
Data corrente: 	28/05/2019	
Data da última atualização: 	30/10/2019	
Autoria: 	MALUCELLI, L. C.; MATOS, M. de; JORDÃO, C.; LOMONACO, D.; LACERDA, L. G.; CARVALHO FILHO, M. A. da S.; MAGALHAES, W. L. E.	
Afiliação: 	Lucca Centa Malucelli, Doutorando da Universidade Positivo; Mailson de Matos, Doutorando da UFPR; Caroline Jordão, Mestranda da UFPR; Diego Lomonaco, UFCE; Luiz Gustavo Lacerda, Pós-graduando da UEPG; Marco Aurélio da Silva Carvalho Filho, Universidade Positivo; WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF.	
Título: 	Influence of cellulose chemical pretreatment on energy consumption and viscosity of produced cellulose nanofibers (CNF) and mechanical properties of nanopaper.	
Ano de publicação: 	2019	
Fonte/Imprenta: 	Cellulose, v. 26, n. 3, p. 1667-1681, Feb. 2019.	
DOI: 	10.1007/s10570-018-2161-0	
Idioma: 	Inglês	
Conteúdo: 	Lignocellulosic fibers are the main sources for producing nanocellulose, in which mechanical methods are the most appropriate to achieve a high yield and generate low residue. High energy consumption is the major drawback in these processes, although they are the cheapest way to produce nanocellulose. Chemical pretreatment is one approach to further decrease the overall cost during defibrillation; however, the influence over sample viscosity and mechanical properties is yet to be investigated. Here, we study the influence of chemical pretreatments using NaOH and 2,2,6,6-tetramethylpiperidine-1-oxyl (TEMPO) on the mechanical, rheological and structural properties of cellulose nanofibers made from bleached eucalyptus pulp. Modification of samples was evidenced by their respective peaks on FTIR spectra. Sample crystallinity increased after partial hemicellulose and amorphous cellulose removal. In addition, a strong correlation between grinding efficiency and lower energy consumption was observed. However, a mild alkaline treatment may improve fiber strength at the expense of suspension stability and energy consumption. Modified nanofibers presented good potential for enhancing mechanical properties and/or improving suspension stability.	
Palavras-Chave: 	Disintegration; Nanocellulose; Nanofibra; Pretreatments; Processing energy; TEMPO-oxidation.	
Thesagro: 	Alcalinidade; Hemicelulose; Viscosidade.	
Thesaurus Nal: 	Alkalinity; Hemicellulose; Nanofibers; Sodium hydroxide; Viscosity.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (56813-1) - UPC - AP - DD -  -  -  - DIS