Data/hora: 19/06/2024 01:07:15

Biblioteca(s): 	Embrapa Agroenergia.	
Data corrente: 	23/11/2022	
Data da última atualização: 	13/02/2023	
Autoria: 	SERRA, L. A.; CRUZ, R. G. da S.; GUTIERREZ, D. M. R.; CRUZ, A. J. G.; CANIZARES, C. A. T.; CHEN, X.; MOSIER, N.; THOMPSON, D.; ASTON, J.; DOOLEY, J.; SHARMA, P.; DE MARCO, J. L.; ALMEIDA, J. R. M. de; ERK, K.; XIMENES, E.; LADISCH, M. R.	
Afiliação: 	LUANA ASSIS SERRA, PURDUE UNIVERSITY; ROSINEIDE GOMES DA SILVA CRUZ, PURDUE UNIVERSITY; DIANA M. R. GUTIERREZ, PURDUE UNIVERSITY; ANTONIO JOSE GONÇALVES CRUZ, PURDUE UNIVERSITY; CARLOS ALBERTO TORRES CANIZARES, PURDUE UNIVERSITY; XUELI CHEN, PURDUE UNIVERSITY; NATHAN MOSIER, PURDUE UNIVERSITY; DAVID THOMPSON, IDAHO NATIONAL LABORATORY; JOHN ASTON, IDAHO NATIONAL LABORATORY; JAMES DOOLEY, FOREST CONCEPTS LLC; PANKAJ SHARMA, PURDUE UNIVERSITY; JANICE LISBOA DE MARCO, UNIVERSITY OF BRASÍLIA; JOAO RICARDO MOREIRA DE ALMEIDA, CNPAE; KENDRA ERK, PURDUE UNIVERSITY/ SCHOOL OF MATERIALS ENGINEERING; EDUARDO XIMENES, PURDUE UNIVERSITY; MICHAEL R. LADISCH, PURDUE UNIVERSITY.	
Título: 	Screening method for Enzyme-based liquefaction of corn stover pellets at high solids.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Bioresource Technology, v. 363, 127999, Nov., 2022.	
DOI: 	https://doi.org/10.1016/j.biortech.2022.127999	
Idioma: 	Inglês	
Conteúdo: 	Liquefaction of high solid loadings of unpretreated corn stover pellets has been demonstrated with rheology of the resulting slurries enabling mixing and movement within biorefinery bioreactors. However, some forms of pelleted stover do not readily liquefy, so it is important to screen out lots of unsuitable pellets before processing is initiated. This work reports a laboratory assay that rapidly assesses whether pellets have the potential for enzyme-based liquefaction at high solids loadings. Twenty-eight pelleted corn stover (harvested at the same time and location) were analyzed using 20 mL enzyme solutions (3 FPU cellulase/ g biomass) at 30 % w/v solids loading. Imaging together with measurement of reducing sugars were performed over 24-hours. Some samples formed concentrated slurries of 300 mg/mL (dry basis) in the small-scale assay, which was later confirmed in an agitated bioreactor. Also, the laboratory assay showed potential for optimizing enzyme formulations that could be employed for slurry formation.	
Palavras-Chave: 	Biorefinery; Laboratory assay; Lignocellulosic biomass.	
Thesaurus Nal: 	Corn stover; Enzymes; Lignocellulosic wastes.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Agroenergia (CNPAE)	
Exemplares: 	CNPAE - (4117-1) - UPC - AP - DD -  -  -  - DIS