Data/hora: 17/06/2024 01:09:27

Biblioteca(s): | Embrapa Unidades Centrais.
Data corrente: | 21/05/2009
Data da última atualização: | 02/08/2019
Autoria: | BEUTLER, A. N.; CENTURION, J. F.; SILVA, A. P. da; CENTURION, M. A. P. da C.; LEONEL, C. L.; FREDDI, O. da S.
Afiliação: | Amauri Nelson Beutler, Universidade Federal do Pampa/Centro de Ciências Agrárias; José Frederico Centurion, Universidade Estadual Paulista - Unesp/Faculdade de Ciências Agrárias e Veterinárias - FCAV/Departamento de Solos e Adubos; Alvaro Pires da Silva, Universidade de São Paulo/Escola Superior de Agricultura Luiz de Queiroz/Departamento de Ciência do Solo; Maria Aparecida Pessôa da Cruz Centurion, Unesp/FCAV/Departamento de Produção Vegetal; Cristian Luarte Leonel, Unesp/FCAV/Departamento de Produção Vegetal; Onã da Silva Freddi, Universidade Estadual Paulista - Unesp/Faculdade de Ciências Agrárias e Veterinárias - FCAV/Departamento de Solos e Adubos.
Título: | Soil compaction by machine traffic and least limiting water range related to soybean yield.
Ano de publicação: | 2008
Fonte/Imprenta: | Pesquisa Agropecuária Brasileira, Brasília, DF, v. 43, n. 11, p. 1591-1600, nov. 2008.
Idioma: | Inglês
Notas: | Título em português: Compactação do solo por tráfego de máquinas e intervalo hídrico ótimo na produtividade de soja.
Conteúdo: | The research aimed to evaluate machine traffic effect on soil compaction and the least limiting water range related to soybean cultivar yields, during two years, in a Haplustox soil. The six treatments were related to tractor (11 Mg weight) passes by the same place: T0, no compaction; and T1*, 1; T1, 1; T2, 2; T4, 4 and T6, 6. In the treatment T1*, the compaction occurred when soil was dried, in 2003/2004, and with a 4 Mg tractor in 2004/2005. Soybean yield was evaluated in relation to soil compaction during two agricultural years in completely randomized design (compaction levels); however, in the second year, there was a factorial scheme (compaction levels, with and without irrigation), with four replicates represented by 9 m2 plots. In the first year, soybean [Glycine max (L.) Merr.] cultivar IAC Foscarim 31 was cultivated without irrigation; and in the second year, IAC Foscarim 31 and MG/BR 46 (Conquista) cultivars were cultivated with and without irrigation. Machine traffic causes compaction and reduces soybean yield for soil penetration resistance between 1.64 to 2.35 MPa, and bulk density between 1.50 to 1.53 Mg m-3. Soil bulk density from which soybean cultivar yields decrease is lower than the critical one reached at least limiting water range (LLWR =0).
Palavras-Chave: | Glicine max; qualidade física do solo; soil physical quality.
Thesagro: | Manejo do Solo.
Thesaurus Nal: | soil management.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/106160/1/Soil-compaction.pdf
Registro original: | Embrapa Unidades Centrais (AI-SEDE)
Exemplares: | AI-SEDE - (45628-1) - UPE - AP - PP - 630.72081 - P474 -  - DIS