Data/hora: 20/06/2024 11:45:49

Biblioteca(s): | Embrapa Soja.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | A - 1
Data corrente: | 06/12/2011
Data da última atualização: | 03/08/2017
Autoria: | CONTE, O.; LEVIEN, R.; DEBIASI, H.; STURMER, S. L. K.; MAZURANA, M.; MULLER, J.
Afiliação: | OSMAR CONTE, UFRGS; RENATO LEVIEN, UFRGS; HENRIQUE DEBIASI, CNPSO; SIDINEI LEANDRO KLOCKNER STURMER, UFRGS; MICHAEL MAZURANA, UFRGS; JÔNATAN MULLER, UFRGS.
Título: | Soil disturbance index as an indicator of seed drill efficiency in no-tillage agrosystems.
Ano de publicação: | 2011
Fonte/Imprenta: | Soil & Tillage Research, Amsterdam, v. 114, n. 1, p. 37-42, 2011.
DOI: | http://dx.doi.org/10.1016/j.still.2011.03.007
Idioma: | Inglês
Conteúdo: | In no-tillage agroecosystems, furrow openers prepare the seed line to place the seeds and fertilizers, and this event represents a unique opportunity to disturb the soil in this kind of crop system. Shanks are used to promote an appropriate soil physical condition, and, in case of soil compaction problems, shanks are used more frequently and at deeper layers of the soil profile. However, this deeper use causes greater draught and does not appropriately disturb the soil because narrow shanks have limited depth performance (critical depth). Here, we tested the operation of shanks in Oxisol and Alfisol. We assessed the shank performance 618 cm of depth, and we evaluated several soil disturbance parameters, such as area of groove, effective depth, and volume, as well as the demand of power force. Based on this evaluation, we calculated the specific power demand and the disturbance index, which is obtained from the ratio of disturbed area and maximum depth. With increasing depth of operation, the specific power demand increased in both soil types, while the disturbance index remaining approximately constant in the Oxisol and decreasing in the Alfisol. In the latter soil type, the shanks operated at more than 12 cm deep, and the lower disturbance index indicated a loss of efficiency in the soil disturbance. Therefore, the disturbance index is an efficient indicator of both the performance of seed drill shanks and the soil disturbance in no-till systems.
Thesagro: | Solo.
Categoria do assunto: | --
Registro original: | Embrapa Soja (CNPSO)
Exemplares: | CNPSO - (32528-2) - UPC - AP - PP - 12022 -  - 12022 - DIS