Data/hora: 01/06/2024 22:16:30

Biblioteca(s): | Embrapa Florestas.
Tipo da produção científica: | Artigo em Anais de Congresso
Data corrente: | 18/11/2014
Data da última atualização: | 18/11/2014
Autoria: | MATTOS, B.; LAZZAROTTO, M.; MAGALHAES, W. L. E.; GATTO, D. A.
Afiliação: | Bruno Dufau Mattos, PIPE, UFPR; MARCELO LAZZAROTTO, CNPF; WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF; Darci Alberto Gatto, Universidade Federal de Pelotas.
Título: | Thermal tools to evaluation of decayed and weathered wood polymer composites prepared by in situ polymerization.
Ano de publicação: | 2014
Fonte/Imprenta: | In: CONGRESSO BRASILEIRO DE ANÁLISE TÉRMICA E CALORIMETRIA, 9., 2014, Serra Negra. Trabalhos. [S.l.]: ABRATEC, 2014.
Páginas: | 6 p.
Descrição Física: | Disponibilizado online.
Idioma: | Inglês
Notas: | CBRATEC.
Conteúdo: | This study aims to apply thermal tools in the evaluation of decayed and weathered wood polymer composites prepared by in situ polymerization of methyl methacrylate (MMA) using glycidyl methacrylate (GMA) and methacrylic acid (MAA) as cross-linkers. The pine wood samples were impregnated in a vacuum/pressure system and polymerized in an oven at 90°C for 10h, using benzoyl peroxide at 1.5 wt% as catalyst. The untreated wood and composites were exposed to in vitro decay tests with Trametes versicolor and Gloeophyllum trabeum fungi, and to artificial weathering. The weight loss after tests was measured, and the characterization was performed by thermogravimetric (TGA) and differential scanning calorimetry (DSC) analysis. The mass loss caused by exposure to fungi was evidently higher in untreated wood in relation to the composites, ~2.5 to 10 times - the composites with GMA and MAA showed the highest resistance to both fungi. The composites without cross-linkers showed the higher mass loss in the artificial weathering tests (>11%), due to the leaching of part of poly(MMA) formed inside wood. By TGA and DSC analysis, we observed shifting in the temperature of thermal events related to polysaccharides and lignin after exposed to decays tests ? more significant changes were for Trametes versicolor tests. The thermograms related to weathered samples showed different results for each composite. The untreated wood and the composite without cross-linker presented loss in lignin, meanwhile the composites with cross-linkers presented degradation in the copolymer formed onto surface of wood. Keywords: TGA, DSC, pinewood, methacrylate, additives
Palavras-Chave: | Compósito; DSC; Metacrilato; Methacrylate; Pinewood; Polímero; TGA.
Thesagro: | Aditivo; Madeira.
Thesaurus Nal: | additives.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/111823/1/2014-MarceloL-CBATC-ThermalTools.pdf
Registro original: | Embrapa Florestas (CNPF)
Exemplares: | CNPF - (53015-1) - UPC - AA - DD -  -  -  - DIS