Data/hora: 24/09/2024 02:12:56

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	21/02/2005	
Data da última atualização: 	03/03/2010	
Autoria: 	MALMONGE, J. A.; ALVES, W. F.; KANDA, D. H. F.; MATTOSO, L. H. C.	
Título: 	Influence of solvents on polyurethane preparation.	
Ano de publicação: 	2004	
Fonte/Imprenta: 	In: WORLD POLYMER CONGRESS-MACRO 2004. Paris, 2004. Anais...Paris, 2004.	
Idioma: 	Inglês	
Conteúdo: 	Polyurethane, characterized by -NH-CO-Q- groups, has been used as a polyrner matrix to produce piezo- and pyroelectric composites [1,2] and blends with conductive polyrners, such as polyaniline doped with p-toluene sulphonic acid(TSA) [3]. During the preparation of polyurethane(PUR) films air bubbles may be formed when using lhe pre-polyrner method (two-step process). We have observed that lhe use of some solvents like N-methyl-2- pyrrolidinone (NMP) and chloroform, drastically diminished these bubbles. In lhe present work we studied lhe influence of NMP and chloroform on lhe chemical reaction of pre-polyrner with polyol during polyurethane (PUR) preparation.	
Palavras-Chave: 	Polímeros; Polímeros condutores; Poliuretano.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8658-1) - UMT - SP - -- - PROCI-04.00135 -  - 2004.00135 - DIS