Data/hora: 17/06/2024 00:45:07

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 29/09/2005
Data da última atualização: | 29/09/2005
Autoria: | MALMONGE, J. A.; CAMPOLI, C. S.; MATTOSO, L. H. C.
Título: | Eletrically conductive blends of polyurethane and polyaniline.
Ano de publicação: | 2001
Fonte/Imprenta: | In: INTERNATIONAL CONFERENCE ON FRONTIERS OF POLYMERS ADVANCED MATERIALS, 6., 2001, Jaboatão dos Guararapes. Technical digest: conference & exhibition: a conference on advanced materials, emerging new technologies and business opportunities. Recife: Universidade Federal de Pernambuco; Buffalo: State University of New York, 2001. p. 107 ref. TuPC22.
Idioma: | Inglês
Conteúdo: | Free standing films of blends from Polyurethane (PU) and polyaniline (PANI) were obtained casting and characterized by the two probe conductivity, in a sandwich configuration with gold electrodes, ultraviolet-visible-near infrared (UV-Vis-NIR) spectoscopy and scanning electronic microscopic (SEM).
Palavras-Chave: | Condutividade; Polianilina; Polímeros.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (8987-1) - UPC - SP - -- - PROCI-01.00082 -  - 2001.00082 - DIS