Data/hora: 23/05/2024 02:15:23

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	23/01/2006	
Data da última atualização: 	23/01/2006	
Autoria: 	MARTINS, M. A.; MATTOSO, L. H. C.	
Título: 	Chemically treated powdered tire rubber for application in composites.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	In: INTERNATIONAL SEMINAR ON ELASTOMERS, 10., 2005, Rio de Janeiro. Resumos... Rio de Janeiro: UERJ, 2005. 1 CD-ROM.	
Idioma: 	Inglês	
Conteúdo: 	Nowadays, considerable efforts have been devoted to finding new applications for ground scrap tires. In this work, the surface of powdered tire rubber has been chemically modified with H2O, H2SO4 and NaOH aqueous solutions in order to increase its adhesion in composite materials. Matrices made from powdered tire rubber have prepared by hot-press molding and characterized by mechanical and dynamic mechanical properties, thermogravimetric analysis, and scanning electron microscopy. The results have shown that the best performance was obtained with matrices treated with NaOH, as it will be discussed.	
Palavras-Chave: 	H2O; H2SO2; NaOH; Thermogravimetric analysis.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9220-1) - UPC - SP - -- - PROCI-05.00063 -  - 2005.00063 - DIS