Data/hora: 24/06/2024 05:55:45

Biblioteca(s): 	Embrapa Gado de Leite.	
Tipo da produção científica: 	Artigo em Periódico Indexado	
Circulação/Nível: 	A - 1	
Data corrente: 	04/04/2022	
Data da última atualização: 	04/04/2022	
Autoria: 	MENDONÇA, H. V. de; OTENIO, M. H.; MARCHÃO, L.; LOMEU, A.; SOUZA, D. S. de; REIS, A.	
Afiliação: 	HENRIQUE VIEIRA DE MENDONÇA, Universidade Federal Rural do Rio de Janeiro; MARCELO HENRIQUE OTENIO, CNPGL; LEONILDE MARCHÃO, Universidade de Trás-os-Montes e Alto Douro; ALICE LOMEU, Universidade Federal Rural do Rio de Janeiro; DENISE SALVADOR DE SOUZA, Universidade Federal Rural do Rio de Janeiro; ALBERTO REIS, Laboratório Nacional de Energia e Geologia de Lisboa.	
Título: 	Biofuel recovery from microalgae biomass grown in dairy wastewater treated with activated sludge: the next step in sustainable production.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Science of the Total Environment, v. 824, 153838, 2022.	
DOI: 	http://dx.doi.org/10.1016/j.scitotenv.2022.153838	
Idioma: 	Inglês	
Conteúdo: 	Microalgae biofuel could be the next step in avoiding the excessive use of fossil fuels and reducing negative impacts on the environment. In the present study, two species of microalgae (Scenedesmus obliquus and Chlorella vulgaris) were used for biomass production, grown in dairy wastewater treated by activated sludge systems. The photobioreactors were operated in batch and in continuous mode. The dry biomass produced was in the range of 2.30 to 3.10 g L&#8722;1. The highest volumetric yields for lipids and carbohydrates were 0.068 and 0.114 g L&#8722;1 day&#8722;1 . Maximum CO2 biofixation (750 mg L&#8722;1 day&#8722;1) was obtained in continuous mode. The maximum values for lipids (21%) and carbohydrates (39%) were recorded in the batch process with species Scenedesmus obliquus. In all of the experiments, the Linolenic acid concentration (C18:3) was greater than 12%, achieving satisfactory oxidative stability and good quality. Projected biofuel production could vary between 4,863,708 kg and 9,246,456 kg year&#8722;1 if all the dairy wastewater produced in Brazil were used for this purpose. Two hectares would be needed to produce 24,99 × 109 L year&#8722;1 of microalgae bioethanol, a far lower value than used in cultivating sugar cane. If all dairy wastewater generated annually in Brazil were used to produce microalgae biomass, it would be possible to obtain approximately 30,609 to 53,647 barrels of biodiesel per year. These data show that only by using dairy wastewater would biofuels be produced to replace 17% to 40% of the fossil fuels currently used in Brazil.	
Palavras-Chave: 	Bioresources; Energia renovável; Renewable energy.	
Thesagro: 	Ácido Graxo; Biocombustível; Biomassa; Laticínio; Microalga.	
Thesaurus Nal: 	Biodiesel; Bioremediation; Fatty acids.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (25611-1) - UPC - AP - DD -  -  -  - DIS