Data/hora: 20/06/2024 16:56:14

Biblioteca(s): | Embrapa Agroindústria Tropical; Embrapa Algodão; Embrapa Unidades Centrais.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | A - 2
Data corrente: | 21/06/2018
Data da última atualização: | 14/03/2019
Autoria: | CRUZ, M. R. da; MORAIS, J. P. S.; MUNIZ, C. R.; ROSA, M. de F.; SOUZA FILHO, M. de S. M. de; AZEREDO, H. M. C. de.
Afiliação: | Mabel Ribeiro da Cruz, Universidade Federal do Ceará/Departamento de Engenharia Química/Campus do Pici; JOAO PAULO SARAIVA MORAIS, CNPA; CELLI RODRIGUES MUNIZ, CNPAT; MORSYLEIDE DE FREITAS ROSA, CNPAT; MEN DE SA MOREIRA DE SOUZA FILHO, CNPAT; HENRIETTE MONTEIRO C DE AZEREDO, CNPAT.
Título: | Mesquite seed gum and Nile tilapia fish gelatin composite films with cellulose nanocrystals.
Ano de publicação: | 2018
Fonte/Imprenta: | Pesquisa Agropecuária Brasileira, Brasília, DF, v. 53, n. 4, p. 495-503, abr. 2018.
Idioma: | Inglês
Notas: | Título em português: Filmes compósitos de galactomanana de algaroba e gelatina de tilápia-do-nilo com nanocristais de celulose.

Conteúdo:

The objective of this work was to determine a suitable combination of the polysaccharide mesquite seed gum (MSG) and the protein Nile tilapia fish gelatin in the composite MSG/gelatin film for food packaging
applications, and to evaluate the effect of cellulose nanocrystals (CNCs) on the film. MSG and gelatin were extracted from mesquite seeds and Nile tilapia residues, respectively, and the CNCs from mesquite pods by
acid hydrolysis. The MSG:gelatin ratio with the best combination of tensile and barrier properties was used to produce the bionanocomposite films, by adding different CNC contents to the MSG/gelatin dispersion. The
MSG:gelatin ratio of 1:1 had a good combination of water vapor permeability (WVP) and tensile strength. The properties of the MSG/gelatin films were improved by the CNCs, mainly at 5 wt%, which produced the highest
tensile strength and modulus, more than 30% higher than those of the control film, and the lowest WVP, 23% lower than that of the control. Higher CNC contents resulted in the aggregation of nanocrystals, impairing
barrier and tensile properties. The nanocomposite film with MSG, gelatin, and CNCs at the respective weight ratios of 1:1:0.1 presents the best overall properties for food packaging applications.

Palavras-Chave: | Bionanocomposites; Bionanocompósitos; Protein.
Thesagro: | Embalagem; Polissacarídeo; Prosopis Juliflora; Proteína.
Thesaurus Nal: | Packaging; Polysaccharides; Proteins.
Categoria do assunto: | --

URL:

http://ainfo.cnptia.embrapa.br/digital/bitstream/item/179594/1/ART18029.pdf
http://ainfo.cnptia.embrapa.br/digital/bitstream/item/178866/1/Mesquite-seed-gum-and-Nile-tilapia-fish-gelatin.pdf

Registro original: | Embrapa Algodão (CNPA)

Exemplares:

AI-SEDE - (62757-1) - UPE - AP - DD -  -  -  - DIS
CNPAT - (15599-1) - UPC - AP - DD -  -  - 2018.0186 - DIS
CNPA - (28651-1) - UPC - AP - DD -  -  -  - DIS