Data/hora: 17/06/2024 11:07:31

Biblioteca(s): | Embrapa Pecuária Sudeste.
Data corrente: | 18/08/2005
Data da última atualização: | 08/05/2023
Autoria: | NASCENTES, C. C.; KAMOGAWA, M. Y.; FERNANDES, K. F.; ARRUDA, M. A. Z.; NOGUEIRA, A. R. de A.; NÓBREGA, J. A.
Afiliação: | CLESIA C. NASCENTE, Universidade Federal de São Carlos; MARCOS Y. KAMOGAWA, Universidade Federal de São Carlos; KELLY G. FERNANDES, Universidade Federal de São Carlos; MARCO A. Z. ARRUDA, Universidade Estadual de Campinas; ANA RITA DE ARAUJO NOGUEIRA, CPPSE; JOAQUIM A. NOBREGA, Universidade Federal de São Carlos.
Título: | Direct determination of Cu, Mn, Pb, Zn in beer by thermospray flame furnace atomic absorption spectrometry.
Ano de publicação: | 2005
Fonte/Imprenta: | Spectrochimica Acta Part B, v. 60, p. 749-753, 2005.
DOI: | https://doi.org/10.1016/j.sab.2005.02.012
Idioma: | Inglês
Conteúdo: | In this work, thermospray flame furnace atomic absorption spectrometry (TS-FF-AAS) was employed for Cu, Mn, Pb, and Zn determination in beer without any sample digestion. The system was optimized and calibration was based on the analyte addition technique. A sample volume of 300 Al was introduced into the hot Ni tube at a flow-rate of 0.4 ml min1 using 0.14 ml -1 nitric acid solution or air as carrier. Different Brazilian beers were directly analyzed after ultrasonic degasification. Results were compared with those obtained by graphite furnace atomic absorption spectrometry (GFAAS). The detection limits obtained for Cu, Mn, Pb, and Zn in aqueous solution were 2.2, 18, 1.6, and 0.9 ug l-1, respectively. The relative standard deviations varied from 2.7% to 7.3% (n=8) for solutions containing the analytes in the 25-50 ug 1-1 range. The concentration ranges obtained for analytes in beer samples were: Cu: 38.0-155 ug l-1; Mn: 110-348 ug l-1, Pb: 13.0-32.9 ug l-1, and Zn: 52.7-226 ug l-1. Results obtained by TS-FF-AAS and GFAAS were in agreement at a 95% confidence level. The proposed method is fast and simple, since sample digestion is not required and sensitivity can be improved without using expensive devices. The TS-FF-AAS presented suitable sensitivity for determination of Cu, Mn, Pb, and Zn in the quality control of a brewery.
Palavras-Chave: | Determination; FAAS; Flame furnace; Spectrometry; Thermospray; Trace metals.
Thesaurus Nal: | Beers.
Categoria do assunto: | W Química e Física
Registro original: | Embrapa Pecuária Sudeste (CPPSE)
Exemplares: | CPPSE - (15809-1) - UPC - AP - DD - PROCI-2005.00103 - NAS - 2005.00103 - DIS