Data/hora: 03/06/2024 13:18:28

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	03/02/2006	
Data da última atualização: 	03/02/2006	
Autoria: 	VENANCIO, E. C.; PATERNO, L. G.; CONSOLIN FILHO, N.; BORATO, C. E.; FIRMINO, A.; MATTOSO, L. H.	
Título: 	Influence of the pH and substrate immersion time on the adsorption of Poly(o-ethoxyaniline) in self-assembled films.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	Journal of the Brazilian Chemical Society, São Paulo, v. 16, n. 3B, p. 558-564, 2005.	
Idioma: 	Inglês	
Conteúdo: 	Ultra-thin films of poly(o-ethoxyaniline)- POEA were deposited onto quartz slides by the self-assembly technique from aqueous solutions of this polymer in pH 3 and 5. The influence of the experimental conditions on the amount of POEA adsorbed was evaluated bu UV-Vis spectroscopy, atomic force microscopy and cyclic voltammetry.	
Palavras-Chave: 	Conducting polymers; Poly(o-ethoxyaniline); Self-assembled films; Thin films.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9383-1) - UPC - SP - -- - PROCI-05.00122 -  - 2005.00122 - DIS