Data/hora: 22/06/2024 06:56:48

Biblioteca(s): | Embrapa Pecuária Sudeste.
Tipo da produção científica: | Resumo em Anais de Congresso
Data corrente: | 10/11/2010
Data da última atualização: | 19/07/2011
Autoria: | GUERRA, M. B. B.; NOGUEIRA, A. R. de A.; SILVA, P. H. T.; PEREIRA FILHO, E. R.
Afiliação: | MARCELO BRAGA BUENO GUERRA, UFSCar/SÃO CARLOS, SP.; ANA RITA DE ARAUJO NOGUEIRA, CPPSE; PATRICIA HELENA TONIOLO SILVA, UFSCar/SÃO CARLOS, SP.; EDENIR RODRIGUES PEREIRA FILHO, UFSCar/SÃO CARLOS, SP.
Título: | Acid digestion for cadmium determination in mineral salt mixing for animal nutrition by thermospra y flame furnace Atomic absorption spectrometry.
Ano de publicação: | 2010
Fonte/Imprenta: | In: RIO SYMPOSIUM ON ATOMIC SPECTROMETRY, 11., 2010, Mar del Prata: Horiba, 2010.
Páginas: | p. 336
Idioma: | Português
Conteúdo: | Cadmium was determined in a sample of mineral salt mixing to milk cattle that has been preparing to be a reference material. A volume of 3 mL of HNO3 3.0 mol L-1 plus 2.0 of H202 30% (W w-1) was added to 250 mg of sample in a cavity microwave oven. After digestion performance the volume was adjusted to 10 mL with water, centrifuged and the supernatant determined by thermospray flame furnace atomic absorption spectrometry (TS-FF-AAS). The system consist of a peristaltic pump, a lab-made commutator injector, and the thermospray flame furnace unit, which includes the ceramic capillary (0.5 mm 10,2.0 mm ED and 100 mm of length) and the Ni tube (10 cm) which is located on the AAS burner. For reaching a higher temperature inside the tube, six holes of 2 mm diameter were drilled in the bottom of the tube. Another orifice was drilled at 90' to the bottom holes for inserting the thermospray capillary. The capillary tip is about 1 mm inside the tube furnace. The manifold was assembled with 0.5 mm i.d. PTFE tubing, sample volume of 1 00 uL, 0.5 mL min-1 of flow rate, and 0.5 % (w v-1) EDTA plus 0.1 % (v v-1) Triton X 100 as carrier stream. Limits of detection (LOD) and quantification (LOQ) 'obtained were 0.31~g L-1 and 1.02~gL-1, respectively. The obtained results were 402 +- 35ug L-1. The accuracy was checked by performing GFAAS (465 +-95ug L-1) and the results proved to be similar by using t test. The high rsd in the GFAAS was probably due the high chloride sample amount.
Palavras-Chave: | Acid digestion; Atomic absorption; Spectrometry.
Thesaurus Nal: | animal nutrition.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/37803/1/PROCI-2010.00194.pdf
Registro original: | Embrapa Pecuária Sudeste (CPPSE)
Exemplares: | CPPSE - (19672-1) - UPC - RA - PP - PROCI-2010.00195 - GUE - 2010.00195 - DIS