Data/hora: 14/06/2024 15:21:56

Biblioteca(s): | Embrapa Instrumentação; Embrapa Soja.
Data corrente: | 07/06/2022
Data da última atualização: | 07/06/2022
Autoria: | VAZ, C. M. P.; RESENDE, J. M. de; FRANCHINI, J. C.; DEBIASI, H.; NUNES, M. R.
Afiliação: | CARLOS MANOEL PEDRO VAZ, CNPDIA; JULIO CEZAR FRANCHINI DOS SANTOS, CNPSO; HENRIQUE DEBIASI, CNPSO.
Título: | Evaluation and recommendations for the use of dynamic penetrometers.
Ano de publicação: | 2022
Fonte/Imprenta: | Soil & Tillage Research, v. 220, 105373, 2022.
ISSN: | 0167-1987
DOI: | https://doi.org/10.1016/j.still.2022.105373
Idioma: | Inglês
Conteúdo: | Dynamic penetrometers are largely used for studies of soil compaction caused by agricultural practices. In this paper, some critical factors affecting precision, operation time, and ease of use of dynamic penetrometers were evaluated. An alternative procedure recording the number of strikes for pre-defined layers (NL) was proposed and compared to the conventional procedure that records depths per strike (Dn). Mass and falling height variability of commercial penetrometers were assessed and the effects on the penetration resistance (PR) equations were evaluated. Comparisons between dynamic and static penetrometers were performed for soils of different textures and a device to extract dynamic penetrometers from very compacted soils was proposed. The alternative procedure-NL presented no statistical difference to the conventional procedure-Dn, shorter acquisition times and simple data post-processing, which was recommended for routine analysis. Mass and falling height variability of 22 Stolf/IAA penetrometers significantly impacted the equations to calculate PR, with variations from &#8722; 5 to +10% compared to the standard equation. Thus, users should utilize their own equations to transform raw data in PR. The dynamic penetrometer performance was significantly affected by soil texture as compared to the static penetrometer. The puller device was effective for extracting the dynamic penetrometers from soils with PR higher than 5 MPa
Palavras-Chave: | Penetration resistance; Penetrometer; Puller device.
Thesagro: | Compactação do Solo; Resistência.
Thesaurus Nal: | Oxisols; Penetrometers; Resistance to penetration; Soil compaction.

Categoria do assunto:

--
X Pesquisa, Tecnologia e Engenharia

Registro original: | Embrapa Instrumentação (CNPDIA)

Exemplares:

CNPDIA - (18008-1) - UPC - AP - DD - PROCI.22/53 -  - 2020/58 - DIS
CNPSO - (40508-1) - UPC - AP - DD -  -  -  - DIS