Data/hora: 17/06/2024 23:20:59

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	05/04/2005	
Data da última atualização: 	05/04/2005	
Autoria: 	RIUL JR. A.; SOTO, A. M. G.; MELLO, S. V.; BONE, S.; TAYLOR, D. M.; MATTOSO, L. H. C.	
Título: 	An electronic tongue using polypyrrole and polyaniline.	
Ano de publicação: 	2003	
Fonte/Imprenta: 	Synthetic Metals, Lausanne, v. 132, p. 109-166, 2003.	
Idioma: 	Inglês	
Conteúdo: 	An electronic tongue composed of six different sensing units: a bare interdigitated electrode, and interdigitated electrodes coated with stearic acid (SA), a polyaniline oligomer (16-mer), polypyrrole (PPy) and mixtures (1:1, w/w) of 16-mer/SA and PPy/SA, was able to distinguish salt, sweet, bitter and acidic solutions. The films were deposited by lhe Langmuir-Blodgett (LB) technique onto interdigitated electrodes, and impedance studies were performed over lhe frequency range 20-105 Hz. The sensor is able to distinguish between different brands of mineral water, tea and coffee and can algo differentiate tastants below lhe human detection thfeshold, proving that conducting polymers are useful sensing materiaIs and transducers for this sort of application. 	
Palavras-Chave: 	Língua eletrônica; Polianilina.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8787-1) - UPC - SP - -- - PROCI-03.00027 -  - 2003.00027 - DIS