Data/hora: 04/06/2024 18:30:14

Biblioteca(s): | Embrapa Amazônia Oriental.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | A - 1
Data corrente: | 03/06/2014
Data da última atualização: | 19/10/2022
Autoria: | REICHERT, J. M.; BERVALD, C. M. P.; RODRIGUES, M. F.; KATO, O. R.; REINERT, D. J.
Afiliação: | José Miguel Reichert, UFSM; Clóvis Moisés Priebe Bervald, GSI Brazil; Miriam Fernanda Rodrigues, UFSM; OSVALDO RYOHEI KATO, CPATU; Dalvan José Reinert, UFSM.
Título: | Mechanized land preparation in eastern Amazon in fire-free forest-based fallow systems as alternatives to slash-and-burn practices: Hydraulic and mechanical soil properties.
Ano de publicação: | 2014
Fonte/Imprenta: | Agriculture, Ecosystems & Environment, v. 192, p. 47-60, July 2014.
DOI: | http://dx.doi.org/10.1016/j.agee.2014.03.046
Idioma: | Inglês
Conteúdo: | Soils of the Brazilian Amazon are particularly fragile due to the inherent soil properties, climate conditions, and the management systems adopted in the region. The aim of this study was to evaluate changes in the mechanical properties and water retention of soils under different tillage systems of secondary vegetation in an area kept fallow for 10 years in Eastern Amazon, Brazil. The treatments consisted of the slash-and-burn of secondary vegetation (SB), slash-and-burn, stump removal and plowing (SBSP), chop-and-mulch of secondary vegetation (CM), and original secondary vegetation (OSV). Undisturbed soil samples were collected immediately, and 15 and 30 days after site preparation (0, 15, and 30 DAP, respectively) to determine bulk density (BD), total porosity (TP) and marcoporosity (Mac), and water retention. Preconsolidation pressure (&#963;p) and compression index (Cc) were assessed at 0 and 15 DAP, whereas soil penetration resistance (PR) was measured directly in the soil profile. The least BD and greatest Mac and TP and the highest water retention at &#8722;30 kPa matric potential were obtained immediately after preparation using the SBSP system. The &#963;p at 0 DAP was lower than the pressure exerted on the soil surface by the machines used for the CM and SBSP systems, but increased numerically to 15 DAP. The PR differed among the systems until reaching 0.25 cm soil depth. Leaving plant residues from the mulching of secondary vegetation on the soil is not, by itself, an effective practice for maintaining structural soil quality in the short term. Soil tillage in the SBSP system decompacts the upper soil layer, which improves all physical indicators, but only in the short term (less than one month). Soil reconsolidates quickly with the lack or reduced effect of organic matter on soil structure and system equilibrium.
Palavras-Chave: | Corte e queima; Preparação do solo.
Thesagro: | Estrutura do Solo; Mecânica do Solo; Mecanização; Vegetação Secundária.
Categoria do assunto: | P Recursos Naturais, Ciências Ambientais e da Terra
Registro original: | Embrapa Amazônia Oriental (CPATU)
Exemplares: | CPATU - (49584-1) - UPC - AP - DD -  -  -  - DIS