Data/hora: 02/06/2024 05:32:23

Biblioteca(s): 	Embrapa Cerrados; Embrapa Semiárido.	
Data corrente: 	05/07/2023	
Data da última atualização: 	23/01/2024	
Autoria: 	FERREIRA, T. R.; MAGUIRE, M. S.; SILVA, B. B. da; NEALE, C. M. U.; SERRÃO, E. A. O.; FERREIRA, J. D.; MOURA, M. S. B. de; SANTOS, C. A. C. dos; SILVA, M. T.; RODRIGUES, L. N.; CARVALHO, H. F. S.	
Afiliação: 	THOMAS R. FERREIRA, UFCG; MITCHELL S. MAGUIRE, Daugherty Water for Food Global Institute at the University of Nebraska, Lincoln, USA; BERNARDO B. DA SILVA, UFCG; CHRISTOPHER M. U. NEALE, Daugherty Water for Food Global Institute at the University of Nebraska, Lincoln, USA; EDIVALDO A. O. SERRÃO, UFCG; JÉSSICA D. FERREIRA, Daugherty Water for Food Global Institute at the University of Nebraska, Lincoln, USA; MAGNA SOELMA BESERRA DE MOURA, CPATSA; CARLOS A. C. DOS SANTOS, UFCG; MADSON T. SILVA, UFCG; LINEU NEIVA RODRIGUES, CPAC; HERICA F. S. CARVALHO, UNIVASF.	
Título: 	Assessment of water demands for irrigation using energy balance and satellite data fusion models in cloud computing: a study in the Brazilian Semiarid region.	
Ano de publicação: 	2023	
Fonte/Imprenta: 	Agricultural Water Management, v. 281, 108260, 2023.	
DOI: 	https://doi.org/10.1016/j.agwat.2023.108260	
Idioma: 	Inglês	
Conteúdo: 	Assessment of irrigation in arid and semiarid regions is imperative to ensure the sustainable use of limited water resources and guarantee food production. Therefore, this study aimed to assess actual evapotranspiration ? ETa derived from the Surface Energy Balance Algorithm for Land ? SEBAL model with and without satellite image fusion as input of a soil water balance in a pilot area of sugarcane in the semiarid region of Brazil. A fusion of Landsat sensors? and Moderate Resolution Imaging Spectroradiometer ? MODIS? images was completed through a Spatial and Temporal Adaptive Reflectance Fusion Model ? STARFM script developed using cloud computing, and its performance in estimating key variables for the radiation balance was evaluated. ETa and irrigation were daily estimated between June, 2015 and May, 2016 by combining STARFM with SEBAL and evaluated according to the Bowen ratio technique and irrigation data. In addition, one-minute surface meteorological elements at the satellite overpass times were used. STARFM performed well with RMSE of 17.00 W m n addition, one-minute surface meteorological elements at the satellite overpass times were used. STARFM performed well with RMSE of 17.00 W m. 2.28 K, 0.07, and 0.01 for Rn, Ts, NDVI, and albedo, respectively. The metrics employed to evaluate ETa estimates indicated that the SEBAL+STARFM has low mean errors PBIAS = -2.75% and RMSE = 0.97 mm d and 16.66 mm month) and high coefficient of determination (0.87 for daily ETa?ET24, and 0.91 for monthly ETa), in comparison with SEBAL using Landsat-only images (PBIAS = -5.25%, RMSE = 0.97 mm d and 17.66 mm month , r2 = 0.92). Adding fused images resulted in a better fit of the estimated cumulative ET24 curve to the measured ET24. The water balance indicated that the cultivated cane suffered water stress, which was better represented by estimates using the ET24 curve with the addition of fused images than Landsat images alone. Although this increase in temporal resolution of the estimated ET24 data indicated a greater water consumption, it informs a quantity that would be sufficient to meet the water demand of the crops.	
Palavras-Chave: 	Água certa; Google earth engine; Semiárido.	
Thesagro: 	Balanço de Energia; Evapotranspiração; Irrigação.	
Thesaurus Nal: 	Energy balance; Evapotranspiration; Remote sensing; Water rights.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Semiárido (CPATSA)	
Exemplares: 	CPATSA - (60486-1) - UPC - AP - DD -  -  -  - DIS
CPAC - (37708-1) - UPC - AP - DD - DIGITAL -  - DIGITAL - DIS