Data/hora: 16/06/2024 22:44:41

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	21/01/2005	
Data da última atualização: 	08/03/2010	
Autoria: 	VAZ, C. M. P.	
Título: 	Use of a combined penetrometer-TDR moisture probe for soil compaction studies.	
Ano de publicação: 	2004	
Fonte/Imprenta: 	In: Invited presentations college on soil physics 2003. [Trieste]: s.n., 2004. p. 451-457.	
Série: 	(ictp lecture notes, 18)	
Idioma: 	Inglês	
Notas: 	Editores: GABRIELS, D. M. ; GHIRARDI, G. ; NIELSEN, D. R. ; SENTIS, I. P. ; SKIDMORE, E. L.	
Conteúdo: 	Soil mechanical strength is an imporant soil parameter that affects root growth and water movement, and controls nutrient and contaminant transport below the rooting zone. The most common way to assess soil strength is by using a soil penetrometer, which characterizes the force needed penetration resitance (PR) depends on such soil properties as bulk density, water content and potential, texture, aggregation, cementation and mineralogy.	
Thesagro: 	Física do Solo; Solo.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8608-1) - UPC - SP - -- - PROCI-04.00095 -  - 2004.00095 - DIS