Data/hora: 13/06/2024 07:21:44

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 29/05/2003
Data da última atualização: | 07/05/2008
Autoria: | VENÂNCIO, T.; AZEREDO, R. B. V.; ENGELSBER, M.; COLNAGO, L. A.
Afiliação: | Instituto de Química de São Carlos, São Carlos, SP; Embrapa Instrumentação Agropecuária, São Carlos, SP; Departamento de Física, Universidade Federal de Pernambuco, Recife, PE.
Título: | Water suppression in high resolution-1H NMR spectroscopy using continuous wave free precession sequence.
Ano de publicação: | 2003
Fonte/Imprenta: | In: ENCONTRO DE USUÁRIOS DE RESSONÂNCIA MAGNÉTICA NUCLEAR, 9., 2003, Angra dos Reis. Extended abstracts... Angra dos Reis> AUREMN, 2003.
Páginas: | 2 f.
Idioma: | Português
Conteúdo: | Here a new method for solvent signal suppression is proposed. It consists on a new pulse sequence named CWFP (continuous wave free precession) which has been successfully used in analytical applications and flow measurments. In this technique the spin system is submitted to a train of pulses with same phase intensity and duration, and separated by time (Tp) <<T2. This sequence produces a excitation profile similar to Jump-return and binomial pulse sequences, with a null in the zero frequency offset.
Palavras-Chave: | Continuour wave; CWFP; Espectroscopia; HR-NMR spectroscopy; Ressonância magnética nuclear; Solvent signal suppression.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (7528-1) - UPC - SP - -- - PROCI-03.00011 -  - 2003.00011 - DIS