Data/hora: 27/07/2024 02:18:37

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	03/12/2004	
Data da última atualização: 	08/03/2010	
Autoria: 	MARTINS, M. A.; MATTOSO, L. H. C.	
Título: 	Short sisal fiber-reinforced tire rubber composites: dynamic and mechanical properties.	
Ano de publicação: 	2004	
Fonte/Imprenta: 	Journal of Applied Polymer Science, New York, v.91, p.670-677, 2004.	
Idioma: 	Inglês	
Conteúdo: 	The world tendency toward using recycled materials demands new procucts from vegetable resources and waste polymers. In this work, composites made from powdered tire rubber (average particle size: 320 um) and sisal fiber were prepared by hot-press molding and investigated by means of dynamic mechanical thermal analysis and tensile properties. The effects of fiber length and content, chemical treatments, and temperature on dynamic mechanical and tensile properties . The effects of fiber lenght and content, chemical treatments, and temperature on dynamic mechanical and tensile properties of such composites were studied. The results showed that mercerization / acetylation treatment of the fibers improves composite performance. Under the conditions investigated the optimurn fiber length 00- tained for tire rubber matrix was 10 mm. Storage and loss moduli both increased with increasing fiber contento The results of this study are encouraging, demonstrating that use of tire rubber and sisal fiber in composites offers promising potential for nonstructural applications.	
Palavras-Chave: 	Composites; Mechanical; Properties; Sisal fibers; Viscoelastic properties.	
Thesaurus Nal: 	rubber.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8519-1) - UPC - SP - -- - PROCI-04.00043 -  - 2004.00043 - DIS