Data/hora: 27/05/2024 06:39:14

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	27/03/2006	
Data da última atualização: 	27/03/2006	
Autoria: 	SIMÕES, M.; ASSIS, O. B. G.; AVACA, L. A.	
Título: 	Electrochemical characterization of sol-gel protective ZrO2 coatings on sintered stainless steels.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	In: INTERNATIONAL LATIN-AMERICAN CONFERENCE ON POWDER TEHNOLOGY-PTECH, 2., 1999, Foz do Iguaçu. PTECH'99: powder technology: challenges for the next millenium. [S. l.]: Associação Brasileira de Cerâmica, 1999. Não-paginado, ref. MO88.	
Idioma: 	Inglês	
Conteúdo: 	ZrO2 films derived from Sol-Gel technique were obtained by dip-coatings onto commercial sintered AlSi 304 and 316 stainless steel compositions. The coatings were processed from a sirconium (4) propoxide precursor solution, sinterized at 800 °C for 2 hours in air.	
Palavras-Chave: 	Electrochemical corrosion; Passive coating; Sol-gel; Surface analysis.	
Thesaurus Nal: 	microscopy.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9661-1) - UPC - SP - -- - PROCI-99.00141 -  - 1999.00141 - DIS