Data/hora: 01/06/2024 14:34:36

Biblioteca(s): 	Embrapa Florestas.	
Data corrente: 	26/05/1993	
Data da última atualização: 	26/05/1993	
Autoria: 	BRITO, J. O.; BARRICHELO, L. E. G.	
Título: 	Caracteristicas do Eucalipto como combustivel: analise quimica imediata da madeira e da casca	
Ano de publicação: 	1978	
Fonte/Imprenta: 	IPEF, Piracicaba, n.16, p.63-70, 1978	
ISSN: 	0100-4557	
Idioma: 	Português	
Conteúdo: 	The purpose of this paper has been to study the proportion of volatile matter, fixed carbon, and ash in the wood and bark of various Eucalyptus species. These analyses are important to a material used as fuel. The proportion of volatile components and fixed carbon influences the burning characteristic of a fuel, because the volatile components are driven off when heated and burn rapidly in the gaseous phase, and fixed carbon burns slowly in the solid phase-like charcoal. The following conclusions could be drawn: a) Significant difference was detected with respect to the volatile mater and fixed carbon between wood and bark. b) Eucalyptus bark, in general, has more fixed carbon and less volatile matter than their respective wood. c) The Eucalyptus cloesiana wood presented the higher fixed carbon (23,3%); in regards to the volatile matter, Eucalyptus grandis presented higher percentage (89,9%), followed by Eucalyptus microcorys (86,2%). d) The ash content of the bark of Eucalyptus species was higher than that of the wood.	
Thesagro: 	Combustível.	
Thesaurus Nal: 	Eucalyptus; fuels.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (8634-1) - ADC - AP - -- -  -  -  - DIS