Data/hora: 14/06/2024 04:00:33

Biblioteca(s): 	Embrapa Agroenergia.	
Data corrente: 	15/03/2019	
Data da última atualização: 	18/11/2019	
Autoria: 	RIBEIRO, R. A.; COLODETTE, J. L.; VAZ JUNIOR, S.	
Afiliação: 	Robisnéa Adriana Ribeiro; Jorge Luiz Colodette; SILVIO VAZ JUNIOR, CNPAE.	
Título: 	Effect of residual effective alkali on eucalyptus kraft pulp yield and chemistry.	
Ano de publicação: 	2018	
Fonte/Imprenta: 	Cerne, v. 24, n. 4, p. 56-64, 2018.	
Idioma: 	Inglês	
Conteúdo: 	The impact of residual effective alkali (REA) and pulp deligniÀ cation degree on Eucalyptus kraft pulp yield and chemistry was investigated. In this study four types of eucalypt clones were evaluated. The eucalypt woods were cooked to kappa numbers of 14± 1, 18± 1, 22± 1 and 26± 1 using two different ranges of REA, namely: low-REA (1-2 g.L-1) and high-REA (8-9 g.L-1). In general, the low-REA cooks lead to pulps of higher yield, viscosity and xylans content and lower brightness and hexenuronic acid (HexA) content, in relation to the high-REA cooks. In addition, the low-REA cooks required about 20% less effective alkali to achieve the target kappa, in spite of demanding about 50% more H-factor. Similar trends were observed for the other woods and kappa values evaluated, but the level of gains varied substantially among woods and deligniÀ cation degrees. Among the various woods, E. globulus was the easiest to delignify. There was a trend of higher brown pulp yield for the cooks terminated at higher kappa in the range of 14-26, but the lignin-HexA free screen yields were about similar in the kappa range of 18-26 for a given wood type.	
Palavras-Chave: 	Kappa number.	
Thesaurus Nal: 	Eucalyptus; Yields.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/194318/1/SILVIO-EFFECT-OF-RESIDUAL.pdf	
Registro original: 	Embrapa Agroenergia (CNPAE)	
Exemplares: 	CNPAE - (3448-1) - UPC - AP - DD -  -  -  - DIS