Data/hora: 12/06/2024 03:44:38

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	26/11/2004	
Data da última atualização: 	08/03/2010	
Autoria: 	RIUL JR. A.; SOUSA, H. C. de; MALMEGRIM, R. R.; SANTOS JR. D. S. DOS; CARVALHO, A. C. P. L. F.; FERNANDO, J. F.; OLIVEIRA JR. O. N.; MATTOSO, L. H. C.	
Título: 	Wine classification by taste sensors made from ultra-thin films and using neural networks.	
Ano de publicação: 	2004	
Fonte/Imprenta: 	Sensors and Actuators . B, Chemical, Lausanne, v.98, p. 77-82, 2004.	
Idioma: 	Inglês	
Conteúdo: 	This paper reports on a sensor array able to distinguish tastes and used to classify red wines. The array comprises sensing units made from Langmuir-Blodgett (LB) films of conducting polymers and lipids and layer-by-Iayer (LBL) films from chitosan deposited onto gold interdigitated electrodes. Using impedance spectroscopy as the principie of detection, we show that distinct clusters can be identified in principal component analysis (PCA) plots for six types ofred wine. Distinction can be made with regard to vintage, vineyard and brands of the red wine. Furthermore, if the data are treated with artificial neural networks (ANNs), this "artificial tongue" can identify wine samples stored under different conditions. This is illustrated by considering 900 wine samples, obtained with 30 measurements for each of the five bottles of the six wines, which could be recognised with 100% accuracy using thealgorithms Standard Backpropagation and Backpropagation momentum in the ANNs.	
Palavras-Chave: 	Polímeros condutores; Trabalho neural.	
Thesagro: 	Sabor; Vinho.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8478-1) - UPC - SP - -- - PROCI-04.00030 -  - 2004.00030 - DIS