Data/hora: 10/06/2024 13:35:13

Biblioteca(s): 	Embrapa Florestas.	
Data corrente: 	05/11/2009	
Data da última atualização: 	24/02/2015	
Autoria: 	MAGALHÃES, W. L. E.; XIAODONG, C.; LUCIA, L. A.	
Afiliação: 	WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF; XIAODONG CAO, SOUTH CHINA UNIVERSITY OF TECHNOLOGY; LUCIAN A. LUCIA, NORTH CAROLINA STATE UNIVERSITY.	
Título: 	Cellulose nanocrystals: celulose core-in-shell nanocomposite assemblies.	
Ano de publicação: 	2009	
Fonte/Imprenta: 	Langmuir, v. 25, n. 22, p. 13250-257, set. 2009.	
Idioma: 	Inglês	
Conteúdo: 	We report herein for the first time how a co-electrospinning technique can be used to overcome the issue of orienting cellulose nanocrystals within a neat cellulose matrix.Ahome-built co-electrospinning apparatus was fabricated that was comprised of a high-voltage power supply, two concentric capillary needles, and one screw-type pump syringe. Eucalyptus-derived cellulose was dissolved inN-methylmorpholine oxide (NMMO) at 120 C and diluted with dimethyl sulfoxide (DMSO) which was used in the external concentric capillary needle as the shell solution. A cellulose nanocrystal suspension obtained by the sulfuric acid hydrolysis of bleached sisal and cotton fibers was used as the core liquid in the internal concentric capillary needle. Three flow rate ratios between the shell and core, four flow rates for the shell dope solution, and four high voltages were tested. The resultant co-electrospun composite fibers were collected onto a grounded metal screen immersed in cold water. Micrometer and submicrometer cellulose fiber assemblies were obtained which were reinforced with cellulose nanocrystals and characterized by FESEM, FTIR, TGA, and XRD. Surprisingly, it was determined that the physical properties for the cellulose controls are superior to the composites; in addition, the crystallinity of the controls was slightly greater.	
Palavras-Chave: 	Nanotecnologia.	
Thesagro: 	Celulose.	
Categoria do assunto: 	W Química e Física	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (46086-1) - UPC - AP - DD -  -  -  - DIS