Data/hora: 06/06/2024 12:38:34

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 13/03/2006
Data da última atualização: | 13/03/2006
Autoria: | HOMEM, M. R. P.; MASCARENHAS, N. D. A.; CRUVINEL, P. E.
Título: | A method for nondestructive testing using multiple energy CT and statistical pattern classification.
Ano de publicação: | 1999
Fonte/Imprenta: | In: ANNUAL MEETING AND EXHIBITION, 44., 1999, Denver, Colorado, USA. Proceedings... Denver, Colorado: SPIE, 1999.
Idioma: | Inglês
Conteúdo: | This paper reports on how multiple energy tecniques in X and gamma-ray CT scanning are able to provide good results with the use of Statistical Pattern Classifcation theory. We obtained a set of four images with different energies (40, 60, 85 and 662 keV) containing aluminum, phosphorus, calcium, water and plexiglass, with a minitomograph scanner for soil science.
Palavras-Chave: | Kappa Coefficient; Nuclear Science; Statistical Pattern Recognition.
Thesaurus Nal: | computed tomography; soil science.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9568-1) - UPC - SP - -- - PROCI-99.0002 -  - 1999.00072 - DIS