Data/hora: 10/06/2024 16:09:10

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 23/03/2006
Data da última atualização: | 23/03/2006
Autoria: | PIZA, M. A.; PATERNO, L. G.; MATTOSO, L. H. C.; COLNAGO, L. A.
Título: | Characterization of electrically conductive blends of collagen and poly (o-ethoxyaniline) by AFM.
Ano de publicação: | 1999
Fonte/Imprenta: | In: INTERNATIONAL CONFERENCE ON SCANNING PROBE MICROSCOPY OF POLYMERS, 1., 1999, Santa Barbara. Abstract book and program... Santa Barbara: University of California, 1999. Não-paginado, ref. P56.
Idioma: | Inglês
Conteúdo: | In this work we report the characterization of electrically conductive blends of collagen and poly (o-ethoxyaniline) by AFM. The roughness increases as a function of the increase in the concentration of conducting polymer in the blend for both de-doped and doped films.
Palavras-Chave: | AFM; Blends; POEA; Polímero.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9648-1) - UPC - SP - -- - PROCI-99.00130 -  - 1999.00130 - DIS