Data/hora: 15/06/2024 02:42:51

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	12/12/2005	
Data da última atualização: 	06/05/2008	
Autoria: 	TORRE-NETO, A.; SCHUELLER, J. K.; HAMAN, J. K.	
Título: 	Automated system for variable rate microsprinkler irrigation in citrus: a demostration unit.	
Ano de publicação: 	2001	
Fonte/Imprenta: 	In: EUROPEAN CONFERENCE ON PRECISION AGRICULTURE-ECPA, 3.; EUROPEAN CONFERENCE OF THE EUROPEAN FEDERATION FOR INFORMATION TECHNOLOGY IN AGRICULTURE, FOOD AND ENVIRONMENT-EFITA, 3., 2001, Montpellier. Third European Conference... Montpellier: Ecole National Supérieure Agronomique, 2001. p. 725-730. 1 CD-ROM.	
Idioma: 	Inglês	
Conteúdo: 	An automated system was developed using soil probes with temperature and matric potencial sensors to measure spatially-variable soil conditions and to spatially-variably control microsprinkler irrigation by local or remote operation using an Rs-485 network. The system was successfully constructed, installed, and demonstrated in a small citrus grove. 	
Palavras-Chave: 	RS-485; Sensors.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9076-1) - UPC - SP - -- - PROCI-01.00149 -  - 2001.00149 - DIS