Data/hora: 31/05/2024 06:22:25

Biblioteca(s): 	Embrapa Agricultura Digital.	
Data corrente: 	25/04/2011	
Data da última atualização: 	08/07/2011	
Autoria: 	VIEIRA, S. R.; CARVALHO, J. R. P. de; PAZ GONZÁLEZ, A.	
Afiliação: 	SIDNEY ROSA VIEIRA, IAC; JOSE RUY PORTO DE CARVALHO, CNPTIA; ANTONIO PAZ GONZÁLEZ, Universidade da Coruña, Espanha.	
Título: 	Jack knifing for semivariogram validation.	
Ano de publicação: 	2010	
Fonte/Imprenta: 	Bragantia, Campinas, v. 69, p. 97-105, 2010	
Idioma: 	Inglês	
Notas: 	Suplemento.	
Conteúdo: 	The semivariogram function fitting is the most important aspect of geostatistics and because of this the model chosen must be validated. Jack knifing may be one the most efficient ways for this validation purpose. The objective of this study was to show the use of the jack knifing technique to validate geostatistical hypothesis and semivariogram models. For that purpose, topographical heights data obtained from six distinct field scales and sampling densities were analyzed. Because the topographical data showed very strong trend for all fields as it was verified by the absence of a sill in the experimental semivariograms, the trend was removed with a trend surface fitted by minimum square deviation. Semivariogram models were fitted with different techniques and the results of the jack knifing with them were compared. The jack knifing parameters analyzed were the intercept, slope and correlation coefficient between measured and estimated values, and the mean and variance of the errors calculated by the difference between measured and estimated values, divided by the square root of the estimation variances. The ideal numbers of neighbors used in each estimation was also studied using the jack knifing procedure. The jack knifing results were useful in the judgment of the adequate models fitted independent of the scale and sampling densities. It was concluded that the manual fitted semivariogram models produced better jack knifing parameters because the user has the freedom to choose a better fit in distinct regions of the semivariogram.	
Palavras-Chave: 	Erro reduzido; Estacionaridade; Semivariograms; Stationarity.	
Thesagro: 	Topografia.	
Thesaurus Nal: 	Topography.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/33101/1/Jack2.pdf	
Registro original: 	Embrapa Agricultura Digital (CNPTIA)	
Exemplares: 	CNPTIA - (15689-1) - UPC - AP - DD -  -  -  - DIS